{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Sound pressure level","Heating","","Nom.","dBA","","49.0"]
["","Cooling","","Nom.","dBA","","49.0"]
["Standard Accessories","Drain plug","","","","1","1"]
["","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","General safety precautions","","","","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Charge","","","kg","","0.76"]
["","Type","","","","","R-32"]
["Operation range","Cooling","Ambient","Max.","°CDB","","50 (4), 46 (5)"]
["","","","Min.","°CDB","","-10"]
["Piping connections","Level difference","IU - OU","Max.","m","","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)"]
["Dimensions","Unit","","Width","mm","","840"]
["","","","Depth","mm","","350"]
["","","","Height","mm","","552"]
["Compressor","Type","","","","","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Frequency","","","Hz","","50"]
["","Voltage","","","V","","220-240"]
["Notes","","","","","(1) - Only possible in combination with ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Contains fluorinated greenhouse gases"]
["","","","","","(2) - Only possible in combination with ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - See separate drawing for operation range"]
["","","","","","","(3) - See separate drawing for electrical data"]
["","","","","","","(4) - Only possible in combination with ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Only possible in combination with ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Dimensions","Unit","","Height","mm","552"]
["","","","Width","mm","840"]
["","","","Depth","mm","350"]
["Weight","Unit","","","kg","32"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","-10"]
["","","","Max.","°CDB","50 (4), 46 (5)"]
["Sound pressure level","Cooling","","Nom.","dBA","46.0"]
["","Heating","","Nom.","dBA","47.0"]
["Refrigerant","Charge","","","kg","0.76"]
["","Charge","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Piping connections","Piping length","OU - IU","Max.","m","20"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","15"]
["Power supply","Frequency","","","Hz","50"]