{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":10,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L"]
[]
[]
[]
[]
["","","","","","ARXS50L2V1B","ARXS60L2V1B","ARXS71L2V1B","ARXS25L2V1B (Archived)","ARXS35L2V1B (Archived)"]
["Sound pressure level","Heating","","High","dBA","","","","47","48"]
["","","","Nom.","dBA","","49","52"]
["","Cooling","","High","dBA","","","","46","48"]
["","","","Nom.","dBA","","49","52"]
["Standard Accessories","Drain plug","","","","1","1","1","1","1"]
["","Installation manual","","","","1","1","1","1","1"]
["","Refrigerant charge label","","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","1","1","1"]
["Refrigerant","Charge","","","TCO2Eq","","","","2.1","2.5"]
["","GWP","","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Charge","","","kg","","1.50","1.70","1.0","1.2"]
["","Type","","","","","R-410A","R-410A","R-410A","R-410A"]
["Fan motor","Speed","Cooling","Super low","rpm","","","","780","780"]
["","","Heating","Super low","rpm","","","","740","740"]
["Operation range","Cooling","Ambient","Max.","°CDB","","46","46","46","46"]
["","","","Min.","°CDB","","-10","-10","10","10"]
["","Heating","Ambient","Max.","°CWB","","18","18","18","18"]
["","","","Min.","°CWB","","-15","-15","-15","-15"]
["Piping connections","Level difference","IU - OU","Max.","m","","20.0","20.0","15","15"]
["","Additional refrigerant charge","","","kg/m","","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)","0.02 (for piping length exceeding 10m)"]
["Sound power level","Cooling","","","dBA","","62","65"]
["","Heating","","","dBA","","62","65"]
["Dimensions","Unit","","Width","mm","","825","825","765","765"]
["","","","Depth","mm","","300","300","285","285"]
["","","","Height","mm","","735","735","550","550"]
["Compressor","Type","","","","","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor","Hermetically sealed swing compressor"]
["Weight","Unit","","","kg","","47","47","34","34"]
["Fan","Air flow rate","Heating","Super low","cfm","","","","904","904"]
["","","","Super low","m³/min","","","","25.6","25.6"]
["","","Cooling","Super low","m³/min","","","","30.1","30.1"]
["","","","Super low","cfm","","","","1,063","1,063"]
["Power supply","Phase","","","","","1~","1~","1~","1~"]
["","Frequency","","","Hz","","50","50","50","50"]
["","Voltage","","","V","","220-230-240","220-230-240","220-240","220-240"]
["Notes","","","","","(1) - 220V","","","(1) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected.","(1) - When connected with multi-system outdoor unit, refer to the specifications of the multi outdoor unit to be connected."]
["","","","","","(2) - 230V","","","(2) - 220V","(2) - 220V"]
["","","","","","(3) - 240V","","","(3) - 230V","(3) - 230V"]
["","","","","","","","","(4) - 240V","(4) - 240V"]
["","","","","","","","","(5) - Contains fluorinated greenhouse gases","(5) - Contains fluorinated greenhouse gases"]
["Fan","Air flow rate","Cooling","Super low","m³/min","48.9"]
["","","Heating","Super low","m³/min","43.1"]
["","","","Super low","cfm","1727"]
["","","Heating","Super low","cfm","1522"]
["Dimensions","Unit","","Height","mm","735"]
["","","","Width","mm","825"]
["","","","Depth","mm","300"]
["Weight","Unit","","","kg","47"]
["Fan motor","Speed","Cooling","Super low","rpm","670"]
["","","Heating","Super low","rpm","670"]
["Compressor","Type","","","","Hermetically sealed swing compressor"]
["Operation range","Cooling","Ambient","Min.","°CDB","10"]
["","","","Max.","°CDB","46"]
["","Heating","Ambient","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Sound pressure level","Cooling","","High","dBA","48"]
["","Heating","","High","dBA","48"]
["Refrigerant","Type","","","","R-410A"]
["","Charge","","","kg","1.7"]
["","Charge","","","tCO2Eq","3.5"]
["","GWP","","","","2087.5"]
["Piping connections","Piping length","OU - IU","Max.","m","30"]
["","Additional refrigerant charge","","","kg/m","0.02 (for piping length exceeding 10m)"]
["","Level difference","IU - OU","Max.","m","20"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50"]
["","Voltage","","","V","220-240"]
["Notes","","","","","","(1) - Contains fluorinated greenhouse gases","(1) - Contains fluorinated greenhouse gases"]