{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":10,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B"]
["Power input","Cooling","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Heating","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Casing","Colour","","","","White","White","White","White","White"]
["Dimensions","Unit","","Height","mm","286","286","286","286","286"]
["","","","Width","mm","770","770","770","770","770"]
["","","","Depth","mm","225","225","225","225","225"]
["Weight","Unit","","","kg","8.5","8.5","8.5","8.5","9"]
["Fan","Air flow rate","Cooling","High","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","","Medium","m³/min","7.8","7.8","8","8","8.2"]
["","","","Low","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Silent operation","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Heating","High","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","","Medium","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","","Low","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Silent operation","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Sound power level","Cooling","","","dBA","55","55","55","55","58"]
["","Heating","","","dBA","55","55","55","55","58"]
["Sound pressure level","Cooling","","High","dBA","39","39","40","40","43"]
["","","","Medium","dBA","33","33","33","33","34"]
["","","","Low","dBA","25","25","26","26","27"]
["","","","Silent operation","dBA","20","20","20","20","20"]
["","Heating","","High","dBA","39","39","40","40","43"]
["","","","Medium","dBA","34","34","34","34","35"]
["","","","Low","dBA","28","28","28","28","29"]
["","","","Silent operation","dBA","23","23","23","23","26"]
["Piping connections","Liquid","","OD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","OD","mm","9.5","9.5","9.5","9.5","9.5"]
["","Drain","","","","18","18","18","18","18"]
["Control systems","Infrared remote control","","","","ARC480A11","ARC480A11","ARC480A11","ARC480A11","ARC480A11"]
["","Wired remote control","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Standard Accessories","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Power supply","Name","","","","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequency","","","Hz","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standard Accessories","AAA dry-cell batteries","","","","","2","","2","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2"]