{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":22,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N / 3AMXM-M"]
[]
[]
[]
[]
["","","","","ATXM20N2V1B / ATXM20N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM20N2V1B / ATXM20N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM20N2V1B / ATXM25N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM20N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM20N2V1B / ATXM50N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM25N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM25N2V1B / ATXM25N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM25N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM35N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM20N2V1B / ATXM50N2V1B / 3AMXM52M3V1B","ATXM25N2V1B / ATXM25N2V1B / 3AMXM52M3V1B","ATXM25N2V1B / ATXM25N2V1B / ATXM25N2V1B / 3AMXM52M3V1B","ATXM25N2V1B / ATXM25N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM25N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM25N2V1B / ATXM50N2V1B / 3AMXM52M3V1B","ATXM35N2V1B / ATXM35N2V1B / 3AMXM52M3V1B","ATXM35N2V1B / ATXM50N2V1B / 3AMXM52M3V1B"]
["Cooling capacity","Nom.","","kW","4.00","5.20","5.20","5.20","5.20","4.50","5.20","5.20","5.20","5.20","5.20","5.00","5.20","5.20","5.20","5.20","5.20","5.20"]
["Space cooling","SEER","","","8.50","8.50","8.50","8.50","8.09","8.50","8.50","8.50","8.50","8.50","8.50","8.50","8.50","8.50","8.50","8.50","8.50","8.50"]
["","Annual energy consumption","","kWh/a","165","215","215","214","225","186","215","215","215","215","215","206","215","215","215","214","214","214"]
["","Capacity","Pdesign","kW","4.00","5.20","5.20","5.20","5.20","4.50","5.20","5.20","5.20","5.20","5.20","5.00","5.20","5.20","5.20","5.20","5.20","5.20"]
["","Energy efficiency class","","","A+++","A+++","A+++","A+++","A++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Space heating (Average climate)","Capacity","Pdesign","kW","4.80","5.00","5.00","5.00","5.00","4.80","5.00","5.00","4.80","5.00","4.80","4.80","5.00","5.00","4.80","4.80","5.00","5.00"]
["","SCOP/A","","","4.23","4.60","4.61","4.62","4.76","4.26","4.62","4.63","4.29","4.64","4.46","4.34","4.61","4.64","4.37","4.49","4.36","4.48"]
["","Energy efficiency class","","","A+","A++","A++","A++","A++","A+","A++","A++","A+","A++","A+","A+","A++","A++","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","3.62","4.14","4.15","4.15","4.22","3.63","4.15","4.15","3.72","4.16","3.79","3.65","4.15","4.16","3.73","3.80","3.85","3.93"]
["","Annual energy consumption","","kWh/a","1,588","1,521","1,519","1,514","1,468","1,577","1,514","1,510","1,566","1,507","1,505","1,533","1,505","1,509","1,537","1,495","1,604","1,548"]
["Nominal efficiency","EER","","","4.62","4.27","4.34","4.36","4.45","4.72","4.38","4.41","4.60","4.42","4.72","4.24","4.40","4.42","4.18","4.32","4.22","4.34"]
["","Annual energy consumption","","kWh","433","609","599","596","584","477","594","590","565","588","551","590","591","588","622","602","616","599"]
["","COP","","","4.18","4.81","4.85","4.88","5.20","4.22","4.89","4.93","4.24","4.95","4.36","4.35","4.92","4.95","4.36","4.44","4.40","4.46"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80","6.80"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range","(3) - See separate drawing for operation range"]
["","","","","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data","(4) - See separate drawing for electrical data"]