{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":6,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXP-N9 / ARXP-N"]
[]
[]
[]
[]
["","","","","ATXP20N5V1B9 / ARXP20N5V1B","ATXP35N5V1B9 / ARXP35N5V1B"]
["Outdoor unit","","","","ARXP20N5V1B","ARXP35N5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.3"]
["","Nom.","","kW","2.00","3.50"]
["","Max.","","kW","2.6","4.0"]
["Heating capacity","Min.","","kW","1.30","1.30"]
["","Nom.","","kW","2.50","4.00"]
["","Max.","","kW","3.50","4.80"]
["Nominal efficiency","COP","","","4.77","4.02"]
["","EER","","","3.71","3.46"]
["","Energy labeling Directive","Cooling","","A","A"]
["","","Heating","","A","A"]
["Space cooling","Annual energy consumption","","kWh/a","101","178"]
["","Energy efficiency class","","","A++","A++"]
["","Capacity","Pdesign","kW","2.00","3.50"]
["","SEER","","","6.90","6.90"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","663","847"]
["","Capacity","Pdesign","kW","2.20","2.80"]
["","Energy efficiency class","","","A++","A++"]
["","Pdh Heating capacity at -10°","","kW","1.98","2.32"]
["","SCOP/A","","","4.64","4.62"]
["Notes","","","","(1) - See separate drawing for electrical data","(1) - See separate drawing for electrical data"]
["","","","","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(2) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified"]
["","","","","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(3) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]