{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW (Archived)"]
["Casing","Colour","","","White"]
["","Button cover","","","No"]
["","Operation LED","Colour","","Blue status indicator"]
["Dimensions","Unit","Height","mm","85"]
["","","Width","mm","85"]
["","","Depth","mm","25"]
["","Packed unit","Height","mm","50"]
["","","Width","mm","217"]
["","","Depth","mm","161"]
["Weight","Unit","","kg","0.110"]
["","Packed unit","","kg","0.317"]
["Packing","Material","","","Cardboard"]
["","Weight","","kg","0.0850"]
["LCD","Type","","","100 x 150 dots"]
["","Dimensions","Height","mm","40.7"]
["","","Width","mm","28.0"]
["","Back light","Colour","","White"]
["Ambient temperature","Operation","Min.","°C","-10"]
["","","Max.","°C","52"]
["","Storage","Min.","°C","-20"]
["","","Max.","°C","70"]
["","Relative humidity <","","%","95"]
["Control systems","Class of temperature control","","","VI"]
["","Contribution to seasonal space heating efficiency","","%","4.0"]
["Wiring connections","Wiring length","Max.","m","500"]