{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":13,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHBH-CB"]
[]
[]
[]
[]
["","","","","","EHBH04CB3V","EHBH08CB3VU","EHBH08CB9W","EHBH08CB3V","EHBH11CB3V","EHBH11CB9W","EHBH16CB3V","EHBH16CB9W"]
["Notes","","","","","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - PED unit category: excluded from scope of PED due to article 1, item 3.6 of 97/23/EC","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(1) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation)."]
["","","","","","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Operation area is extended to lower flow rates only in case the unit operates with heat pump only. (Not in startup, no BUH operation, no defrost operation).","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel","(2) - Including piping + PHE + back-up heater; excluding expansion vessel"]
["","","","","","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - Including piping + PHE + back-up heater; excluding expansion vessel","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(3) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)"]
["","","","","","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - DB/WB 7°C/6°C - LWC 35°C (DT=5°C)","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(4) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit."]
["","","","","","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(5) - The sound pressure level is measured in an anechoic room at 1m distance from the unit. It is a relative value, depending on the distance and acoustic environment.The sound pressure level mentioned is maximum possible value inside operation range of unit.","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning","(5) - 15°C-25°C: BUH only no heat pump operation = during commissioning"]
["","","","","","(6) -  > 50°C BSH only, no heatpump","(6) - 15°C-25°C: BUH only, no heat pump operation = during commissioning","(6) -  > 50°C BSH only, no heatpump","(6) -  > 50°C BSH only, no heatpump","(6) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(6) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(6) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models","(6) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","(7) - Lower if back-up heater is installed; In case of no back-up heater, then heat pump operation starts at 10°C","","","(7) -  > 50°C BSH only, no heatpump","(7) -  > 50°C BSH only, no heatpump","(7) -  > 50°C BSH only, no heatpump","(7) -  > 50°C BSH only, no heatpump"]
["","","","","","","(8) - Refer to operation range for detail for differences between *RHQ* and *RLQ* models"]
["","","","","","","(9) - If condensation is expected, the installation of a EKHBDP* drain pan kit must be considered."]
["","","","","","","(10) - > 50°C BSH only, no heatpump operation"]
["","","","","","","(11) - Above mentioned power supply of the hydrobox is for the backup heater only. The switch box and the pump of the hydrobox are supplied via the outdoor unit. The optional domestic hot water tank has a separate power supply."]
["","","","","","","(12) - The switch box and the pump of the hydrobox are supplied via the outdoor unit. The optional domestic hot water tank has a separate power supply."]
["","","","","","","(13) - Equipment complying with EN/IEC 61000-3-12: European/international technical standard setting the limits for harmonic currents produced by equipment connected to public low-voltage system with input current > 16A and ≤ 75A per phase"]
["","","","","","","(14) - Select diameter and type according to national and local regulations"]
["Casing","Colour","","","","White","","White","White","White","White","White","White"]
["","Material","","","","Precoated sheet metal","","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal","Precoated sheet metal"]
["Dimensions","Unit","","Height","mm","890","","890","890","890","890","890","890"]
["","","","Width","mm","480","","480","480","480","480","480","480"]
["","","","Depth","mm","344","","344","344","344","344","344","344"]
["Weight","Unit","","","kg","41.0","","45.0","43.0","43.0","44.0","44.0","45.0"]
["PED","Category","","","","Art3§3, See note 1","","Category I, See note 1","Category I, See note 1","Art3§3, See note 1","Art3§3, See note 1","Art3§3, See note 1","Art3§3, See note 1"]
["Sound power level","Nom.","","","dBA","40.0","","40.0","40.0 (4)","41.0 (4)","41.0 (4)","44.0 (4)","44.0 (4)"]
["Sound pressure level","Nom.","","","dBA","26.0","","26.0","26.0 (5)","27.0 (5)","27.0 (5)","30.0 (5)","30.0 (5)"]
["Operation range","Heating","Water side","Min.","°C","15","","15","15 (6)","15 (6)","15 (6)","15 (6)","15 (6)"]
["","","","Max.","°C","55.0","","55.0","55.0","55.0 (8)","55.0 (8)","55.0 (8)","55.0 (8)"]
["Power supply","Name","","","","See note 11","","See note 11","See note 11","See note 11","See note 11","See note 11","See note 11"]
["Electric heater","Power supply","","Name","","3V3","","9W","3V3","3V3","9W","3V3","9W"]
["","","","Phase","","1~","","Refer to installation manual or drawing 4D093592","1~","1~","Refer to installation manual or drawing 4D093592","1~","Refer to installation manual or drawing 4D093592"]
["","","","Frequency","Hz","50","","50","50","50","50","50","50"]
["","","","Voltage","V","230","","","230","230","","230"]
["Wiring connections","For connection with user interface","","Quantity","","2","","2","2","2","2","2","2"]
["","","","Remark","","0.75 mm² till 1.25 mm² (max length 500m)","","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)","0.75 mm² till 1.25 mm² (max length 500m)"]