{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-A / ARXM-N9"]
[]
[]
[]
[]
["","","","","FAA71AUVEB / ARXM71N2V1B9"]
["Cooling capacity","Nom.","","kW","6.80"]
["","Max.","","kW","6.95"]
["Heating capacity","Nom.","","kW","7.50"]
["","Max.","","kW","7.59"]
["Nominal efficiency","EER","","","3.40"]
["","COP","","","3.19"]
["","Annual energy consumption","","kWh","1000"]
["","Energy labeling Directive","Cooling","","A"]
["","","Heating","","D"]
["Space cooling","Energy efficiency class","","","A+"]
["","Capacity","Pdesign","kW","6.80"]
["","SEER","","","5.77"]
["","Annual energy consumption","","kWh/a","412"]
["Space heating (Average climate)","Energy efficiency class","","","A"]
["","Capacity","Pdesign","kW","4.50"]
["","SCOP/A","","","3.81"]
["","Pdh Heating capacity at -10°","","kW","4.50"]
["","Annual energy consumption","","kWh/a","1652"]
["Energy Efficiency Range","","","","A+++ ~ D"]