{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":7,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ100D2VEB / RZQSG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L9V1B","FBQ125D2VEB / RZQSG125L9V1B"]
["Cooling capacity","Nom.","","kW","9.5 (2)","","12.0 (2)"]
["Space cooling","SEER","","","5.61","5.10","5.47"]
["","Annual energy consumption","","kWh/a","593","652","768"]
["","Capacity","Pdesign","kW","9.50","9.50","12.00"]
["","Energy efficiency class","","","A+","A","A"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","7.60","7.60"]
["","SCOP/A","","","4.15","3.80","4.01"]
["","Energy efficiency class","","","A+","A","A+"]
["","Annual energy consumption","","kWh/a","2,564","2,800","2,653"]
["Nominal efficiency","EER","","","3.35 (1)","","3.23 (1)"]
["","Annual energy consumption","","kWh","1,418","","1,858"]
["","COP","","","3.67 (1)","","3.63 (1)"]
["","Energy labeling Directive","Cooling","","A","","A"]
["","","Heating","","A","","A"]
["Heating capacity","Nom.","","kW","10.80 (2)","","13.50 (2)"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]
["","","","","(3) - Annual energy consumption is according to Energy labeling directive 2002/31/EC","","(3) - Annual energy consumption is according to Energy labeling directive 2002/31/EC"]
["","","","","(4) - SEER and SCOP are according to EN 14825","","(4) - SEER and SCOP are according to EN 14825"]
["","","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]