{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":10,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXC-D / RXC-D"]
[]
[]
[]
[]
["","","","","FTXC20DV1B / RXC20DV1B","FTXC25DV1B / RXC25DV1B","FTXC35DV1B / RXC35DV1B","FTXC50DV1B / RXC50DV1B","FTXC60DV1B / RXC60DV1B","FTXC71DV1B / RXC71DV1B"]
["Outdoor unit","","","","RXC20DV1B","RXC25DV1B","RXC35DV1B","RXC50DV1B","RXC60DV1B","RXC71DV1B"]
["Cooling capacity","Min.","","kW","1.3","","1.3","1.4","1.8","2.3"]
["","Max.","","kW","3.0","","4.0","6.2","7.0","7.3"]
["Heating capacity","Min.","","kW","1.30","","1.30","1.36","1.48","2.30"]
["","Max.","","kW","4.00","","4.80","6.60","8.00","9.00"]
["Nominal efficiency","COP","","","3.73","","3.74","3.71","3.81","3.25"]
["","EER","","","3.36","","3.35","3.29","3.30","2.98"]
["","Energy labeling Directive","Cooling","","A","","A","A","A","C"]
["","","Heating","","A","","A","A","A","C"]
["Space cooling","Annual energy consumption","","kWh/a","106","","175","276","339","460"]
["","Energy efficiency class","","","A++","","A++","A++","A++","A"]
["","Capacity","Pdesign","kW","2.08","","3.44","5.08","6.21","6.96"]
["","SEER","","","6.89","","6.87","6.45","6.40","5.30"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","595","","733","1,234","1,353","2,332"]
["","Capacity","Pdesign","kW","1.87","","2.24","3.90","4.10","6.35"]
["","Energy efficiency class","","","A+","","A+","A+","A+","A"]
["","Pdh Heating capacity at -10°","","kW","1.38","","1.71","2.99","3.49","5.36"]
["","SCOP/A","","","4.40","","4.28","4.42","4.24","3.81"]
["Cooling capacity","Min.","","kW","","1.3"]
["","Max.","","kW","","3.0"]
["Heating capacity","Min.","","kW","","1.30"]
["","Max.","","kW","","4.00"]
["Nominal efficiency","EER","","","","3.35"]
["","COP","","","","3.79"]
["","Energy labeling Directive","Cooling","","","A"]
["","","Heating","","","A"]
["Space cooling","Energy efficiency class","","","","A++"]
["","Capacity","Pdesign","kW","","2.57"]
["","SEER","","","","6.84"]
["","Annual energy consumption","","kWh/a","","131"]
["Space heating (Average climate)","Energy efficiency class","","","","A+"]
["","Capacity","Pdesign","kW","","2.23"]
["","SCOP/A","","","","4.45"]
["","Pdh Heating capacity at -10°","","kW","","1.57"]
["","Annual energy consumption","","kWh/a","","701"]
["Energy Efficiency Range","","","","","A+++ ~ D"]