{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-F / RXF-F"]
[]
[]
[]
[]
["","","","","FTXF20F5V1B / RXF20F5V1B","FTXF25F5V1B / RXF25F5V1B","FTXF35F5V1B / RXF35F5V1B","FTXF42F5V1B / RXF42F5V1B","FTXF50F5V1B / RXF50F5V1B"]
["Outdoor unit","","","","RXF20F5V1B","RXF25F5V1B","RXF35F5V1B","RXF42F5V1B","RXF50F5V1B"]
["Cooling capacity","Min.","","kW","1.3","1.30","1.30","1.4","1.30"]
["","Nom.","","kW","2","2.50","3.30","4.2","5"]
["","Max.","","kW","2.4","2.80","3.80","4.3","5.30"]
["Heating capacity","Min.","","kW","1.3","1.30","1.30","1.4","1.43"]
["","Nom.","","kW","2.4","2.80","3.50","4.6","5.40"]
["","Max.","","kW","3.3","3.70","4.40","5","6.13"]
["Nominal efficiency","EER","","","3.38","3.24","3.30","3.3","3.30"]
["","COP","","","3.75","3.73","3.72","3.71","3.71"]
["","Annual energy consumption","","kWh","108","135","188","226","269"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","2","2.50","3.50","4.2","5"]
["","SEER","","","6.5","6.50","6.50","6.5","6.50"]
["","Annual energy consumption","","kWh/a","108","135","188","226","269"]
["Space heating (Average climate)","Energy efficiency class","","","A+","A+","A+","A+","A+"]
["","Capacity","Pdesign","kW","2.2","2.40","2.60","3.3","3.80"]
["","SCOP/A","","","4.2","4.20","4.20","4.3","4.10"]
["","Pdh Heating capacity at -10°","","kW","1.86","1.97","2.21","2.61","3.24"]
["","Annual energy consumption","","kWh/a","733","801","867","1,075","1,297"]
["Notes","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m. Data for high efficiency series, Eurovent certified"]
["","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m. Data for standard efficiency series"]
["","","","","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data","(3) - See separate drawing for electrical data"]