{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":8,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXN-L / RXN-L"]
[]
[]
[]
[]
["","","","","FTXN25LV1B / RXN25LV1B","FTXN35LV1B / RXN35LV1B","FTXN50LV1B / RXN50LV1B","FTXN60LV1B / RXN60LV1B"]
["Cooling capacity","Min.","","kW","1.30","1.30","1.88","2.00"]
["","Max.","","kW","2.80","3.50","6.20","6.50"]
["","Nom.","","kW","2.50","3.20","5.45","6.21"]
["Space cooling","SEER","","","4.88","5.05","4.70","4.61"]
["","Annual energy consumption","","kWh/a","180","222","406","472"]
["","Capacity","Pdesign","kW","2.50","3.20","5.45","6.21"]
["","Energy efficiency class","","","B","B","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","1.91","2.35","4.40","4.48"]
["","SCOP/A","","","3.61","3.81","3.46","3.48"]
["","Energy efficiency class","","","A","A","A","A"]
["","Annual energy consumption","","kWh/a","741","864","1,780","1,802"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","OD","mm","9.52","9.52","12.70","15.90"]
["","Drain","OD","mm","16.5","16.5","16.5","16.5"]
["Nominal efficiency","EER","","","3.21","3.22","3.21","3.22"]
["","Annual energy consumption","","kWh","390","498","850","965"]
["","COP","","","3.61","3.61","3.61","3.62"]
["","Energy labeling Directive","Cooling","","A","A","A","A"]
["","","Heating","","A","A","A","A"]
["Heating capacity","Nom.","","kW","2.80","3.50","5.62","6.40"]
["","Min.","","kW","1.30","1.30","1.32","1.56"]
["","Max.","","kW","3.70","4.00","6.60","7.10"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]