{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":7,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / RXP20M5V1B","FTXP25M5V1B9 / RXP25M5V1B","FTXP35M5V1B9 / RXP35M5V1B"]
["Outdoor unit","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Cooling capacity","Min.","","kW","","1.3"]
["","Nom.","","kW","","2.50"]
["","Max.","","kW","","3.0"]
["Heating capacity","Min.","","kW","","1.30"]
["","Nom.","","kW","","3.00"]
["","Max.","","kW","","4.00"]
["Nominal efficiency","Annual energy consumption","","kWh","","326"]
["","COP","","","","4.36"]
["","EER","","","","3.83"]
["","Energy labeling Directive","Cooling","","","A"]
["","","Heating","","","A"]
["Space cooling","Annual energy consumption","","kWh/a","","126"]
["","Energy efficiency class","","","","A++"]
["","Capacity","Pdesign","kW","","2.50"]
["","SEER","","","","6.92"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","","728"]
["","Capacity","Pdesign","kW","","2.40"]
["","Energy efficiency class","","","","A++"]
["","Pdh Heating capacity at -10°","","kW","","2.10"]
["","SCOP/A","","","","4.61"]
["Notes","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","(3) - See separate drawing for electrical data"]
["Cooling capacity","Min.","","kW","1.3","","1.3"]
["","Nom.","","kW","2.00","","3.50"]
["","Max.","","kW","2.6","","4.0"]
["Heating capacity","Min.","","kW","1.30","","1.30"]
["","Nom.","","kW","2.50","","4.00"]
["","Max.","","kW","3.50","","4.80"]
["Nominal efficiency","EER","","","4.02","","3.49"]
["","COP","","","4.77","","4.02"]
["","Annual energy consumption","","kWh","249"]
["","Energy labeling Directive","Cooling","","A","","A"]
["","","Heating","","A","","A"]
["Space cooling","Energy efficiency class","","","A++","","A++"]
["","Capacity","Pdesign","kW","2.00","","3.50"]
["","SEER","","","6.79","","6.62"]
["","Annual energy consumption","","kWh/a","103","","186"]
["Space heating (Average climate)","Energy efficiency class","","","A++","","A++"]
["","Capacity","Pdesign","kW","2.20","","2.80"]
["","SCOP/A","","","4.65","","4.64"]
["","Pdh Heating capacity at -10°","","kW","1.99","","2.33"]
["","Annual energy consumption","","kWh/a","662","","845"]
["Energy Efficiency Range","","","","A+++ ~ D","","A+++ ~ D"]