{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":13,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20N5V1B / RXP20M5V1B","FTXP25N5V1B / RXP25M5V1B","FTXP35N5V1B / RXP35M5V1B","FTXP50N2V1B / RXP50M5V1B","FTXP50N2V1B / RXP50M2V1B","FTXP60N2V1B / RXP60M5V1B","FTXP60N2V1B / RXP60M2V1B","FTXP71N2V1B / RXP71M2V1B","FTXP71N2V1B / RXP71M5V1B"]
["Outdoor unit","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Cooling capacity","Min.","","kW","","","","1.7","1.7","1.7","1.7","2.3","2.3"]
["","Nom.","","kW","","","","5.0","5.0","6.0","6.0","7.1","7.1"]
["","Max.","","kW","","","","6.0","6.0","7.0","7.0","7.3","7.3"]
["Heating capacity","Min.","","kW","","","","1.7","1.7","1.7","1.7","2.3","2.3"]
["","Nom.","","kW","","","","6.0","6.0","7.0","7.0","8.2","8.2"]
["","Max.","","kW","","","","7.7","7.7","8.0","8.0","9.0","9.0"]
["Nominal efficiency","Annual energy consumption","","kWh","","","","693","693","912","912","1,345","1,345"]
["","COP","","","","","","3.80","3.80","3.63","3.63","3.19","3.19"]
["","EER","","","","","","3.61","3.61","3.29","3.29","2.64","2.64"]
["","Energy labeling Directive","Cooling","","","","","A","A","A","A","D","D"]
["","","Heating","","","","","A","A","A","A","D","D"]
["Space cooling","Annual energy consumption","","kWh/a","","","","240","240","308","308","401","401"]
["","Energy efficiency class","","","","","","A++","A++","A++","A++","A++","A++"]
["","Capacity","Pdesign","kW","","","","5.0","5.0","6.0","6.0","7.1","7.1"]
["","SEER","","","","","","7.30","7.30","6.82","6.82","6.20","6.20"]
["Space heating (Average climate)","Annual energy consumption","","kWh/a","","","","1,463","1,463","1,638","1,638","2,166","2,166"]
["","Capacity","Pdesign","kW","","","","4.60","4.60","4.80","4.80","6.20","6.20"]
["","Energy efficiency class","","","","","","A+","A+","A+","A+","A+","A+"]
["","Pdh Heating capacity at -10°","","kW","","","","3.15","3.15","3.29","3.29","4.24","4.24"]
["","SCOP/A","","","","","","4.40","4.40","4.10","4.10","4.01","4.01"]
["Notes","","","","","","","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m.","(1) - Nominal cooling capacities are based on: indoor temperature: 27°CDB, 19°CWB, outdoor temperature: 35°CDB, equivalent refrigerant piping: 5m, level difference: 0m."]
["","","","","","","","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m.","(2) - Nominal heating capacities are based on: indoor temperature: 20°CDB, outdoor temperature: 7°CDB, 6°CWB, equivalent refrigerant piping: 5m, level difference: 0m."]
["Cooling capacity","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2.00","2.50","3.50"]
["","Max.","","kW","2.6","3.0","4.0"]
["Heating capacity","Min.","","kW","1.30","1.30","1.30"]
["","Nom.","","kW","2.50","3.00","4.00"]
["","Max.","","kW","3.50","4.00","4.80"]
["Nominal efficiency","EER","","","3.75","3.75","3.26"]
["","COP","","","4.77","4.36","4.02"]
["","Energy labeling Directive","Cooling","","A","A","A"]
["","","Heating","","A","A","A"]
["Space cooling","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","2.00","2.50","3.50"]
["","SEER","","","7.20","7.20","7.20"]
["","Annual energy consumption","","kWh/a","97","121","170"]
["Space heating (Average climate)","Energy efficiency class","","","A++","A++","A++"]
["","Capacity","Pdesign","kW","2.20","2.40","2.80"]
["","SCOP/A","","","4.65","4.61","4.64"]
["","Pdh Heating capacity at -10°","","kW","1.99","2.09","2.35"]
["","Annual energy consumption","","kWh/a","663","728","845"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]