{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FUQ71CVEB / RZQG71L7Y1B9","FUQ71CVEB / RZQG71L7V1B","FUQ100CVEB / RZQG100L7V1B","FUQ100CVEB / RZQG100L7Y1B","FUQ100CVEB / RZQG100LY1B","FUQ125CVEB / RZQG125L7V1B","FUQ125CVEB / RZQG125L7Y1B"]
["Cooling capacity","Nom.","","kW","6.8","6.8","9.5","9.5","9.5","12.0","12.0"]
["Space cooling","SEER","","","6.23","6.23","5.62","5.62","5.62","5.03","5.03"]
["","Annual energy consumption","","kWh/a","840","382.022","591.637","592","591.637","834.99","834.99"]
["","Capacity","Pdesign","kW","6.80","6.80","9.50","9.5","9.50","12.00","12.00"]
["","Energy efficiency class","","","A++","A++","A+","A+","A+","B","B"]
["Space heating (Average climate)","Capacity","Pdesign","kW","7.60","7.60","11.30","11.3","11.30","14.13","14.13"]
["","SCOP/A","","","4.08","4.08","3.93","3.93","3.93","4.44","4.44"]
["","Energy efficiency class","","","A+","A+","A","A","A","A+","A+"]
["","Annual energy consumption","","kWh/a","2,607","2,607","4,027","4,027","4,027","4,456","4,456"]
["Nominal efficiency","EER","","","4.07","4.07","4.08","4.08","4.08","3.40","3.40"]
["","Annual energy consumption","","kWh","840","840","1,230","1,230","1,230","1,770","1,770"]
["","COP","","","4.47","4.47","4.04","4.04","4.04","4.04","4.04"]
["","Energy labeling Directive","Cooling","","A","A","A","A","A","A","A"]
["","","Heating","","A","A","A","A","A","A","A"]
["Heating capacity","Nom.","","kW","7.5","7.5","10.8","10.8","10.8","13.5","13.5"]
["Notes","","","","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only","(1) - EER/COP according to Eurovent 2012, for use outside EU only"]
["","","","","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load","(2) - Nominal efficiency: cooling at 35°/27° nominal load, heating at 7°/20° nominal load"]