{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":11,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWG-AF"]
[]
[]
[]
[]
["","","","","","FWG05AAFNMV1","FWG05AF","FWG08AAFNMV1","FWG08AF","FWG11AAFNMV1","FWG11AF"]
["Sound pressure level","Low","","","dBA","23 (5)","23 (5)","37 (6)","37 (6)","41 (6)","41 (6)"]
["","High","","","dBA","37 (5)","37 (5)","47 (6)","47 (6)","51 (6)","51 (6)"]
["Total sound power level","Low","","","dBA","34 (4)","34 (4)","49 (4)","49 (4)","49 (4)","49 (4)"]
["","High","","","dBA","46 (4)","46 (4)","57 (4)","57 (4)","59 (4)","59 (4)"]
["Water flow","Cooling","","Low","l/h","770","770","1,250","1,250","1,570","1,570"]
["","","","High","l/h","770","770","1,250","1,250","1,570","1,570"]
["","Heating","","High","l/h","670","670","970","970","1,360","1,360"]
["","","","Low","l/h","670","670","970","970","1,360","1,360"]
["","Water pressure drop","Heating","High","kPa","18","18","27","27","42","42"]
["","","","Low","kPa","9","9","15","15","24","24"]
["","","Cooling","High","kPa","18","18","19","19","32","32"]
["","","","Low","kPa","9","9","10","10","19","19"]
["Piping connections","Drain","","OD","mm","19","19","19","19","19","19"]
["","Water","","Inlet","","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\""]
["","","","Outlet","","3/4\"","3/4\"","3/4\"","3/4\"","3/4\"","3/4\""]
["Power input","High","","","kW","0.047","0.047","0.100","0.100","0.130","0.130"]
["","Low","","","kW","0.02","0.02","0.04","0.04","0.05","0.05"]
["Dimensions","Unit","","Width","mm","820","820","820","820","820","820"]
["","","","Depth","mm","820","820","820","820","820","820"]
["","","","Height","mm","265","265","268","268","300","300"]
["Casing","Colour","","","","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint","Without powder paint"]
["Weight","Unit","","","kg","26.0","26.0","28.0","28.0","32.0","32.0"]
["Fan","Air flow rate","","Low","m³/h","","595 (3)","","951 (3)","","1,155 (3)"]
["","","","High","m³/h","","1,053 (3)","","1,512 (3)","","1,801 (3)"]
["Cooling capacity (standard conditions)","Sensible capacity 2-pipe","","Low","kW","2.23 (1)","2.23 (1)","3.78 (1)","3.78 (1)","4.86 (1)","4.86 (1)"]
["","","","High","kW","3.81 (1)","3.81 (1)","5.66 (1)","5.66 (1)","7.05 (1)","7.05 (1)"]
["","Total capacity 2-pipe","","Low","kW","2.79 (1)","2.79 (1)","4.97 (1)","4.97 (1)","6.46 (1)","6.46 (1)"]
["","","","High","kW","4.36 (1)","4.36 (1)","7.11 (1)","7.11 (1)","8.88 (1)","8.88 (1)"]
["Decoration panel","Dimensions","Unit","Height","mm","85","85","85","85","85","85"]
["","","","Depth","mm","990","990","990","990","990","990"]
["","","","Width","mm","990","990","990","990","990","990"]
["Heating capacity (standard conditions)","Capacity 2-pipe","","High","kW","6.74 (2)","6.74 (2)","9.86 (2)","9.86 (2)","13.79 (2)","13.79 (2)"]
["","","","Low","kW","4.45 (2)","4.45 (2)","7.09 (2)","7.09 (2)","10.09 (2)","10.09 (2)"]
["Current input","High","","","A","0.26","0.26","0.74","0.74","0.95","0.95"]
["","Low","","","A","0.13","0.13","0.28","0.28","0.35","0.35"]
["Power supply","Type","","","","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50","230 /  1 /  50"]
["","Phase","","","","1N~","1N~","1N~","1N~","1N~","1N~"]
["","Frequency","","","Hz","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Fan motor","Power input","","Low","kW","0.220","0.220","0.036","0.036","0.049","0.049"]
["","","","High","kW","0.470","0.470","0.100","0.100","0.130","0.130"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K.","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; entering water temp. 7°C, water temperature rise 5K."]
["","","","","","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C","(2) - Heating: 2 pipe: air 20°CDB; entering water 50°C"]
["","","","","","(3) - Air flow at 0Pa ESP","(3) - Air flow at 0Pa ESP","(3) - Air flow at 0Pa ESP","(3) - Air flow at 0Pa ESP","(3) - Air flow at 0Pa ESP","(3) - Air flow at 0Pa ESP"]
["","","","","","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741","(4) - Sound power level according to ISO3741"]
["","","","","","(5) - Sound pressure level measured at 1.4m below the facia (JIS C 9612).","(5) - Sound pressure level measured at 1.4m below the facia (JIS C 9612).","(5) - Sound pressure level measured at 1.4m below the facia (JIS C 9612).","(5) - Sound pressure level measured at 1.4m below the facia (JIS C 9612).","(5) - Sound pressure level measured at 1.4m below the facia (JIS C 9612).","(5) - Sound pressure level measured at 1.4m below the facia (JIS C 9612)."]
["","","","","","(6) - Sound pressure measured at 1,5m below the facia (JIS B 8615)","(6) - Sound pressure measured at 1,5m below the facia (JIS B 8615)","(6) - Sound pressure measured at 1,5m below the facia (JIS B 8615)","(6) - Sound pressure measured at 1,5m below the facia (JIS B 8615)","(6) - Sound pressure measured at 1,5m below the facia (JIS B 8615)","(6) - Sound pressure measured at 1,5m below the facia (JIS B 8615)"]