{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":12,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXAA-A"]
[]
[]
[]
[]
["","","","","","FXAA15AUV1B","FXAA20AUV1B","FXAA25AUV1B","FXAA32AUV1B","FXAA40AUV1B","FXAA50AUV1B","FXAA63AUV1B"]
["Sound pressure level","Heating","","At high fan speed","dBA","33.0","34.0","36.0","38.5","38.0","42.0","47.0"]
["","","","At low fan speed","dBA","28.5","28.5","28.5","28.5","33.5","35.5","38.5"]
["","","","At medium fan speed","dBA","31.0","31.5","32.5","33.5","36.0","39.0","43.0"]
["","Cooling","","At low fan speed","dBA","28.5","28.5","28.5","28.5","33.5","35.5","38.5"]
["","","","At high fan speed","dBA","32.0","33.0","35.0","37.5","37.0","41.0","46.5"]
["","","","At medium fan speed","dBA","30.5","31.0","32.0","33.0","35.5","38.5","42.5"]
["Standard Accessories","Installation and operation manual","","","","1","1","1","1","1","1","1"]
["","Installation plate","","","","1","1","1","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","4","4","4","4","4","4","4"]
["","Heat insulating tape","","","","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.017","0.019","0.028","0.030","0.025","0.033","0.050"]
["","Heating","","At high fan speed","kW","0.025","0.029","0.034","0.035","0.030","0.039","0.060"]
["Cooling capacity","Total capacity","","At high fan speed","kW","1.7","2.2","2.8","3.6","4.5","5.6","7.1"]
["Piping connections","Liquid","","OD","mm","6","6","6","6","6","6","6"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Gas","","OD","mm","9.52","9.52","9.52","9.52","12.70","12.70","12.70"]
["","","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection"]
["","Drain","","","","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)","VP13 (I.D. 15/O.D. 18)"]
["Sound power level","Cooling","","At high fan speed","dBA","51.0","52.0","53.0","55.0","55.0","58.0","63.0"]
["Air filter","Type","","","","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable","Removable / washable"]
["Dimensions","Unit","","Width","mm","795","795","795","795","1,050","1,050","1,050"]
["","","","Depth","mm","266","266","266","266","269","269","269"]
["","","","Height","mm","290","290","290","290","290","290","290"]
["Casing","Colour","","","","White","White","White","White","White","White","White"]
["Weight","Unit","","","kg","12","12","12","12","15","15","15"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","7.1","7.9","8.3","9.4","12.2","14.2","18.2"]
["","","","At low fan speed","m³/min","6.5","6.5","6.5","6.5","9.8","10.9","12.9"]
["Heating capacity","Total capacity","","At high fan speed","kW","1.9","2.5","3.2","4.0","5.0","6.3","8.0"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6","6","6","6","6","6"]
["Power supply","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Name","","","","V1","V1","V1","V1","V1","V1","V1"]
["","Frequency","","","Hz","50","50","50","50","50","50","50"]
["","Voltage","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Notes","","","","","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB","(1) - Cooling: indoor temp. 27°CDB, 19.0°CWB; outdoor temp. 35°CDB"]
["","","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB"]
["","","","","","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates.","(3) - The sound power level is an absolute value indicating the power which a sound source generates."]
["","","","","","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(4) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%.","(5) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA","(6) - MCA/MFA: MCA = 1.1 x FLA"]
["","","","","","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker","(7) - Instead of a fuse, use a circuit breaker"]
["","","","","","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA","(8) - Select wire size based on the value of MCA"]
["","","","","","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases","(9) - Contains fluorinated greenhouse gases"]