{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":12,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FXMA-A"]
[]
[]
[]
[]
["","","","","","FXMA50A5VEB","FXMA63A5VEB","FXMA80A5VEB","FXMA100A5VEB","FXMA125A5VEB","FXMA200AXVMB","FXMA250AXVMB"]
["Sound pressure level","Heating","","At high fan speed","dBA","","","","","","48.0"]
["","","","At low fan speed","dBA","","","","","","45.0"]
["","","","At medium fan speed","dBA","","","","","","46.5"]
["","Cooling","","At low fan speed","dBA","","","","","","45.0"]
["","","","At high fan speed","dBA","","","","","","48.0"]
["","","","At medium fan speed","dBA","","","","","","46.5"]
["Standard Accessories","Installation and operation manual","","","","1","1","1","1","1","1","1"]
["","Wire clamp material","","","","","","","","","1","1"]
["","Spring washer","","","","","","","","","2","2"]
["","Hexagon head screw","","","","","","","","","2","2"]
["","Plain washer","","","","","","","","","8","8"]
["","Hexagon head screw with washer","","","","","","","","","49","49"]
["","Gas connection pipe","","","","","","","","","1","1"]
["","General safety precautions","","","","","","","","","1","1"]
["Refrigerant","GWP","","","","","","","","","675"]
["","Type","","","","","","","","","R-32"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","","","","","","0.54"]
["","Heating","","At high fan speed","kW","","","","","","0.54"]
["Cooling capacity","Total capacity","","At high fan speed","kW","","","","","","22.4"]
["","Nom.","","","kW","","","","","","22.4"]
["Piping connections","Liquid","","OD","mm","","","","","","9.5"]
["","","","Type","","","","","","","Flare connection"]
["","Gas","","OD","mm","","","","","","19.1"]
["","","","Type","","","","","","","Flange"]
["","Drain","","","","","","","","","BSP1"]
["Required ceiling void >","mm","","","","350","350","350","350","350"]
["Sound power level","Cooling","","At high fan speed","dBA","","","","","","75.0"]
["Dimensions","Unit","","Width","mm","","","","","","1,490"]
["","","","Depth","mm","","","","","","1,100"]
["","","","Height","mm","","","","","","470"]
["Casing","Material","","","","","","","","","Galvanised steel plate"]
["","Colour","","","","","","","","","Unpainted"]
["Weight","Unit","","","kg","","","","","","105"]
["Fan","External static pressure - 50Hz","","High","Pa","","","","","","250"]
["","","","Low","Pa","","","","","","50"]
["","External static pressure - 60Hz","","High","Pa","","","","","","250"]
["","","","Low","Pa","","","","","","50"]
["","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","","","","","","62"]
["","","","At low fan speed","m³/min","","","","","","41"]
["Heating capacity","Total capacity","","At high fan speed","kW","","","","","","25.0"]
["","Nom.","","","kW","","","","","","25.0"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","","","","","","6"]
["Power supply","Phase","","","","","","","","","1~"]
["","Name","","","","","","","","","VM"]
["","Frequency","","","Hz","","","","","","50/60"]
["","Voltage","","","V","","","","","","220-240/220-230"]
["Cooling capacity","Total capacity","","At high fan speed","kW","5.6","7.1","9.0","11.2","14.0","","28.0"]
["Heating capacity","Total capacity","","At high fan speed","kW","6.3","8.0","10.0","12.5","16.0","","31.5"]
["Power input - 50Hz","Cooling","","At high fan speed","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["","Heating","","At high fan speed","kW","0.125","0.14","0.198","0.191","0.254","","0.65"]
["Dimensions","Unit","","Height","mm","300","300","300","300","300","","470"]
["","","","Width","mm","1,000","1,000","1,000","1,400","1,400","","1,490"]
["","","","Depth","mm","700","700","700","700","700","","1,100"]
["Weight","Unit","","","kg","35","35","35","46","46","","115"]
["Casing","Colour","","","","Unpainted","Unpainted","Unpainted","Unpainted","Unpainted","","Unpainted"]
["","Material","","","","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","Galvanised steel plate","","Galvanised steel plate"]
["Fan","Air flow rate - 50Hz","Cooling","At high fan speed","m³/min","18.0","19.5","25.0","32.0","36.0","","74"]
["","","","At low fan speed","m³/min","15.0","16.0","20.0","23.0","26.0","","52"]
["","External static pressure - 50Hz","","High","Pa","200","200","200","200","200","","250"]
["","External static pressure - 60Hz","","High","Pa","200","200","200","200","200","","250"]
["Refrigerant","Type","","","","R-32","R-32","R-32","R-32","R-32","","R-32"]
["","GWP","","","","675","675","675","675","675","","675"]
["Sound power level","Cooling","","At high fan speed","dBA","61.0","64.0","67.0","65.0","70.0","","76.0"]
["Sound pressure level","Cooling","","At high fan speed","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","At medium fan speed","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","At low fan speed","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["","Heating","","At high fan speed","dBA","41.0","42.0","43.0","43.0","44.0","","48.0"]
["","","","At medium fan speed","dBA","39.0","40.0","41.0","41.0","42.0","","46.5"]
["","","","At low fan speed","dBA","37.0","38.0","39.0","39.0","40.0","","45.0"]
["Piping connections","Liquid","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","","Flare connection"]
["","","","OD","mm","6.35","6.35","6.35","9.52","9.52","","9.5"]
["","Gas","","Type","","Flare connection","Flare connection","Flare connection","Flare connection","Flare connection","","Flange"]
["","","","OD","mm","12.7","12.7","12.7","15.9","15.9","","19.1"]
["","Drain","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","","BSP1"]
["Air filter","Type","","","","Resin net","Resin net","Resin net","Resin net","Resin net"]
["Standard Accessories","Washer for hanger bracket","","","","8","8","8","8","8"]
["","Drain hose","","","","1","1","1","1","1"]
["","Insulation for fitting","","","","2","2","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","1","1"]
["","Screws","","","","16","16","16","16","16"]
["","Sealing pad","","","","3","3","3","3","3"]
["Power supply","Name","","","","VE","VE","VE","VE","VE","","VM"]
["","Phase","","","","1~","1~","1~","1~","1~","","1~"]
["","Frequency","","","Hz","50/60","50/60","50/60","50/60","50/60","","50/60"]
["","Voltage","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","","220-240/220-230"]
["Current - 50Hz","Maximum fuse amps (MFA)","","","A","6","6","6","6","6","","6"]
["Fan","External static pressure - 50Hz","","Low","Pa","","","","","","","50"]
["","External static pressure - 60Hz","","Low","Pa","","","","","","","50"]