{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC30YV"]
[]
[]
[]
[]
["","","","","","MC30YVM"]
["Type","","","","","Air Purifier"]
["Application","","","","","Floor standing type"]
["Casing","Colour","","","","White"]
["Dimensions","Unit","","Height","mm","450"]
["","","","Width","mm","270"]
["","","","Depth","mm","270"]
["Weight","Unit","","","kg","5.8"]
["Applicable room area","m²","","","","23 (1), 46 (2)"]
["CADR","m³/h","","","","180"]
["Air purifying operation","Power input","","Turbo","kW","0.025"]
["","","","M","kW","0.015"]
["","","","Silent","kW","0.008"]
["Sound pressure level","Air purifying operation","","Turbo","dBA","37"]
["","","","Medium","dBA","27"]
["","","","Silent","dBA","19"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","180"]
["","","","Medium","m³/h","120"]
["","","","Silent","m³/h","60"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Standard Accessories","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Operation manual","","","","1"]
["Power cord","m","","","","1.8"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Running current","Air purifying operation","","Turbo","A","0.13"]
["","","","Medium","A","0.09"]
["","","","Silent","A","0.08"]
["Notes","","","","","(1) - The applicable room area is appropriate for operating the unit of maximum fan speed (HH). Applicable room area indicates  the space where a certain amount of dust particles can be remover in 30 minutes. (JEM 1467)"]
["","","","","","(2) - The applicable room area is appropriate for operating  the unit of maximum fan speed (HH). Applicable room area was calculated in accordance with NRCC-54013 standard using cigarette smoke CADR that was tested accoring to JEM1467."]
["","","","","","(3) - Converted to CADR standards from test values in accordance with JEM1467."]
["","","","","","(4) - Operating sound levels are the average of values measured at 1m away from the front, left, right and top of the unit. (These are equal to the values in an anechoic chamber)"]
["","","","","","(5) - Electrostatic HEPA filter is attached in the unit."]
["","","","","","(6) - Other function   :   Auto-restart function"]