{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Type","","","","","Humidifying air purifier"]
["Application","","","","","Floor standing type"]
["Casing","Colour","","","","White (N9. 0)"]
["Dimensions","Unit","","Height","mm","600 (5)"]
["","","","Width","mm","395"]
["","","","Depth","mm","287"]
["Weight","Unit","","","kg","12.5"]
["Applicable room area","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Air purifying operation","Power input","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Silent","kW","0.008"]
["Humidifying operation","Power input","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Silent","kW","0.011"]
["","Water tank capacity","","","l","3.6"]
["Sound pressure level","Air purifying operation","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","","","Low","dBA","27"]
["","","","Silent","dBA","18"]
["","Humidifying operation","","Turbo","dBA","54"]
["","","","Medium","dBA","37"]
["","","","Low","dBA","27"]
["","","","Silent","dBA","23"]
["Fan","Air flow rate","Air purifying operation","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["","","","Low","m³/h","132"]
["","","","Silent","m³/h","60"]
["","","Humidifying operation","Turbo","m³/h","420"]
["","","","Medium","m³/h","210"]
["","","","Low","m³/h","132"]
["","","","Silent","m³/h","102"]
["Dust collecting method","","","","","Electrostatic HEPA filter"]
["Deodorizing method","","","","","Flash streamer + Deodorizing catalyst"]
["Standard Accessories","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Power cord","m","","","","2"]
["Power supply","Phase","","","","1~"]
["","Frequency","","","Hz","50/60"]
["","Voltage","","","V","220-240/220-230"]
["Notes","","","","","(1) - The coverage area is appropriate for operating the unit of maximum fan speed(HH). Coverage area indicates the space where a certain amount of dust particles can be removed in 30 minutes."]
["","","","","","(2) - Converted to NRCC standards from test values in accordance with JEM1467."]
["","","","","","(3) - Operating sound levels are the average of values measured at 1m away from the front, left, right and top of the unit. (These are equal to the values in an anechoic chamber)"]