{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":69,"n_cols":7,"rows_kept":69,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RQEQ-P3"]
[]
[]
[]
[]
["","","","","RQEQ140PY13","RQEQ180PY13","RQEQ212PY13"]
["Standard Accessories","Installation manual","","","Installation manual","Installation manual","Installation manual"]
["","Operation manual","","","Operation manual","Operation manual","Operation manual"]
["","Clamps","","","Clamps","Clamps","Clamps"]
["Operation range","Cooling","Max.","°CDB","43","43","43"]
["","","Min.","°CDB","-5","-5","-5"]
["","Heating","Min.","°CWB","-20","-20","-20"]
["","","Max.","°CWB","15.5","15.5","15.5"]
["Space cooling","B Condition (30°C - 27/19)","Pdc","kW","10.3","13.3","14.7"]
["","","EERd","","4.40","3.86","3.63"]
["","D Condition (20°C - 27/19)","Pdc","kW","5.01","4.94","4.95"]
["","","EERd","","9.29","9.54","9.64"]
["","A Condition (35°C - 27/19)","EERd","","2.54","2.22","1.74"]
["","","Pdc","kW","14.0","18.0","20.0"]
["","C Condition (25°C - 27/19)","EERd","","7.31","6.89","6.57"]
["","","Pdc","kW","6.63","8.53","9.47"]
["Compressor","Type","","","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor","Hermetically sealed scroll compressor"]
["Weight","Unit","","kg","175","175","179"]
["Refrigerant","Charge","","TCO2Eq","21.5","22.1","23.4"]
["","GWP","","","2,087.5","2,087.5","2,087.5"]
["","Charge","","kg","10.3","10.6","11.2"]
["","Type","","","R-410A","R-410A","R-410A"]
["Cooling capacity","Prated,c","","kW","14.0","18.0","20.0"]
["","Nom.","","kW","14.0 (1)","18.0 (1)","21.2 (1)"]
["Space heating (Average climate)","TOL","COPd (declared COP)","","1.92","1.84","1.64"]
["","","Pdh (declared heating cap)","kW","8.5","10.6","11.9"]
["","D Condition (12°C)","Pdh (declared heating cap)","kW","4.18","4.40","4.44"]
["","","COPd (declared COP)","","6.43","6.82","6.88"]
["","B Condition (2°C)","COPd (declared COP)","","3.42","3.56","3.92"]
["","","Pdh (declared heating cap)","kW","4.58","5.72","6.41"]
["","C Condition (7°C)","COPd (declared COP)","","4.84","5.26","5.40"]
["","","Pdh (declared heating cap)","kW","3.29","3.68","4.12"]
["","A Condition (-7°C)","COPd (declared COP)","","2.20","2.22","2.20"]
["","","Pdh (declared heating cap)","kW","7.52","9.40","10.5"]
["","TBivalent","Pdh (declared heating cap)","kW","8.5","10.6","11.9"]
["","","Tbiv (bivalent temperature)","°C","-10","-10","-10"]
["","","COPd (declared COP)","","1.92","1.84","1.64"]
["Piping connections","Liquid","OD","mm","9.52","9.52","9.52"]
["","","Type","","Braze connection","Braze connection","Braze connection"]
["","Gas","OD","mm","15.9","19.1","19.1"]
["","","Type","","Braze connection","Braze connection","Braze connection"]
["","Discharge gas","OD","mm","12.7","15.9","15.9"]
["","","Type","","Braze connection","Braze connection","Braze connection"]
["Sound power level","Cooling","Nom.","dBA","79","83","87"]
["Dimensions","Unit","Width","mm","635","635","635"]
["","","Depth","mm","765","765","765"]
["","","Height","mm","1,680","1,680","1,680"]
["Heating capacity","Prated,h","","kW","16.0","20.0","22.4"]
["","Nom.","","kW","16.0 (2)","20.0 (2)","22.4 (2)"]
["Power supply","Phase","","","3~","3~","3~"]
["","Name","","","Y1","Y1","Y1"]
["","Frequency","","Hz","50","50","50"]
["","Voltage","","V","380-415","380-415","380-415"]
["Notes","","","","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m","(1) - Cooling: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB; equivalent piping length: 7.5m; level difference: 0m"]
["","","","","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m","(2) - Heating: indoor temp. 20°CDB; outdoor temp. 7°CDB, 6°CWB; equivalent refrigerant piping: 7.5m; level difference: 0m"]
["","","","","(3) - Sound values are measured in an anechoic chamber. Operating sound level generally becomes higher than this value depending on the operating conditions, reflected sound, and peripheral noise.","(3) - Sound values are measured in an anechoic chamber. Operating sound level generally becomes higher than this value depending on the operating conditions, reflected sound, and peripheral noise.","(3) - Sound values are measured in an anechoic chamber. Operating sound level generally becomes higher than this value depending on the operating conditions, reflected sound, and peripheral noise."]
["","","","","(4) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(4) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB","(4) - RLA is based on following conditions: indoor temp. 27°CDB, 19°CWB; outdoor temp. 35°CDB"]
["","","","","(5) - TOCA means the total value of each OC set.","(5) - TOCA means the total value of each OC set.","(5) - TOCA means the total value of each OC set."]
["","","","","(6) - MSC means the maximum current during start up of the compressor","(6) - MSC means the maximum current during start up of the compressor","(6) - MSC means the maximum current during start up of the compressor"]
["","","","","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits.","(7) - Voltage range: units are suitable for use on electrical systems where voltage supplied to unit terminal is not below or above listed range limits."]
["","","","","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%.","(8) - Maximum allowable voltage range variation between phases is 2%."]
["","","","","(9) - Select wire size based on the larger value of MCA or TOCA","(9) - Select wire size based on the larger value of MCA or TOCA","(9) - Select wire size based on the larger value of MCA or TOCA"]
["","","","","(10) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(10) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker).","(10) - MFA is used to select the circuit breaker and the ground fault circuit interrupter (earth leakage circuit breaker)."]
["","","","","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases","(11) - Contains fluorinated greenhouse gases"]