{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":9,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-M"]
[]
[]
[]
[]
["","","","","","2MXM40M2V1B","2MXM40M4V1B","2MXM40M3V1B","2MXM50M2V1B"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","30","","","34"]
["","","Calefacción","Súper baja","m³/min","32","","","34"]
["","","","Súper baja","cfm","1059","","","1200"]
["","","Calefacción","Súper baja","cfm","1130","","","1200"]
["Dimensiones","Unidad","","Altura","mm","550","550","550","550"]
["","","","Anchura","mm","765","765","765","765"]
["","","","Profundidad","mm","285","285","285","285"]
["Peso","Unidad","","","kg","36","36","36","41"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","760","500","500","890"]
["","","Calefacción","Súper baja","rpm","820","320","320","890"]
["Compresor","Type","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10","-10 (2)","-10"]
["","","","Máx.","°CBS","46","46","46 (2)","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15","-15","-15"]
["","","","Máx.","°CBH","18","18","18","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","46","46"]
["","","","Nom.","dBA","48","","","46"]
["","Calefacción","","Alto","dBA","","48","48"]
["","","","Nom.","dBA","50","","","48"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32"]
["","Carga","","","kg","0.88","0.88","0.88","1.15"]
["","Carga","","","tCO2Eq","0.6","0.60","0.59","0.8"]
["","GWP","","","","675","675","675","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20","20 (1)","20"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 20 m)","0,02 (para longitud de tubería superior a 20 m)","0,02 (para longitud de tubería superior a 20 m)","0,02 (para longitud de tubería superior a 20 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","15.0","15.0","15"]
["","","Ud. int. – Ud. int.","Máx.","m","7.5","7.5","7.5","7.5"]
["","Longitud de tubería total","Sistema","Real","m","30","30","30","30"]
["Accesorios estándar","Installation manual","","","","Installation manual","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50"]
["","Tensión","","","V","220-240","220-230-240","220-230-240","220-240"]
["Notas","","","","","","(1) - Para una habitación"]
["","","","","","","","(1) - Para una habitación"]
["","","","","","","","(2) - Consulte la ilustración por separado para el rango de funcionamiento"]
["Accesorios estándar","Reducer assembly","","","","","","","1"]