{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N9"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B9 (Archived)","2MXM50N2V1B9 (Archived)"]
["Dimensiones","Unidad","","Altura","mm","552","552"]
["","","","Anchura","mm","852","852"]
["","","","Profundidad","mm","350","350"]
["Peso","Unidad","","","kg","36","41"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","500","500"]
["","","Calefacción","Súper baja","rpm","320","500"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46","48"]
["","Calefacción","","Alto","dBA","48","50"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","0.88","1.15"]
["","Carga","","","tCO2Eq","0.60","0.78"]
["","GWP","","","","675","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20","20"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 20 m)","0,02 (para longitud de tubería superior a 20 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","15"]
["","","Ud. int. – Ud. int.","Máx.","m","7.5","7.5"]
["","Longitud de tubería total","Sistema","Real","m","30","30"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-230-240","220-230-240"]
["Notas","","","","","(1) - Para una habitación","(1) - Para una habitación"]
["Accesorios estándar","Reducer assembly","","","","","1"]