{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","47"]
["","Refrigeración","","Nom.","dBA","46"]
["Accesorios estándar","Manual de instalación","","","","1"]
["","Bolsa de tornillos","","","","1"]
["","Tapón de drenaje","","","","1"]
["","Tapón de drenaje (1)","","","","6"]
["","Tapón de drenaje (2)","","","","3"]
["","Quite la etiqueta de gases fluorados","","","","1"]
["","Etiqueta de refrigerante adicional","","","","1"]
["Refrigerante","Charge","","","TCO2Eq","1.2"]
["","GWP","","","","675"]
["","Carga","","","kg","1.8"]
["","Tipo","","","","R-32"]
["Motor del vent.","Velocidad","Refrigeración","Súper baja","rpm","420"]
["","","Calefacción","Súper baja","rpm","420"]
["Conexiones de tubería","Diferencia de nivel","Ud. int. – Ud. int.","Máx.","m","7.5"]
["","","Ud. int. – Ud. ext.","Máx.","m","15"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)"]
["","Longitud de tubería total","Sistema","Real","m","50"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado"]
["Dimensiones","Unidad","","Anchura","mm","868"]
["","","","Profundidad","mm","320"]
["","","","Altura","mm","734"]
["Peso","Unidad","","","kg","57"]
["Power supply","Phase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]
["Notas","","","","","(1) - Contiene gases fluorados de efecto invernadero"]
["","","","","","(2) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","(3) - Consulte en el plano independiente con los datos eléctricos."]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","","24"]
["","","Calefacción","Súper baja","m³/min","","24"]
["","","","Súper baja","cfm","","847"]
["","","Calefacción","Súper baja","cfm","","847"]
["Dimensiones","Unidad","","Altura","mm","","734"]
["","","","Anchura","mm","","868"]
["","","","Profundidad","mm","","320"]
["Peso","Unidad","","","kg","","57"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","","420"]
["","","Calefacción","Súper baja","rpm","","420"]
["Compresor","Tipo","","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","","-10"]
["","","","Máx.","°CBS","","46"]
["","Calefacción","Ambiente","Mín.","°CBH","","-15"]
["","","","Máx.","°CBH","","18"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","","46"]
["","Calefacción","","Nom.","dBA","","47"]
["Refrigerante","Tipo","","","","","R-32"]
["","Carga","","","kg","","1.80"]
["","Carga","","","tCO2Eq","","1.2"]
["","GWP","","","","","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","","25"]
["","Carga de refrigerante adicional.","","","kg/m","","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","15"]
["","","Ud. int. – Ud. int.","Máx.","m","","7.5"]
["","Longitud de tubería total","Sistema","Real","m","","50"]
["Accesorios estándar","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Alimentación eléctrica","Fase","","","","","1~"]
["","Frecuencia","","","Hz","","50"]
["","Tensión","","","V","","220-240"]