{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXM-N8"]
[]
[]
[]
[]
["","","","","","3MXM40N2V1B8","3MXM52N2V1B8"]
["Dimensiones","Unidad","","Altura","mm","734","734"]
["","","","Anchura","mm","974","974"]
["","","","Profundidad","mm","401","401"]
["Peso","Unidad","","","kg","57","57"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","420","420"]
["","","Calefacción","Súper baja","rpm","420","420"]
["Compresor","Type","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10"]
["","","","Máx.","°CBS","46","46"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","46","46"]
["","Calefacción","","Nom.","dBA","47.0","47.0"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","1.8","1.8"]
["","Carga","","","tCO2Eq","1.22","1.22"]
["","GWP","","","","675.0","675.0"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","25","25"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15.0","15.0"]
["","","Ud. int. – Ud. int.","Máx.","m","7.5","7.5"]
["","Longitud de tubería total","Sistema","Real","m","50","50"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]
["Notas","","","","","(1) - Para una habitación","(1) - Para una habitación"]
["","","","","","(2) - Para combinación con CVXM-A, FVXM-A, la longitud de tubería máxima es de 30 m.","(2) - Para combinación con CVXM-A, FVXM-A, la longitud de tubería máxima es de 30 m."]