{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":62,"n_cols":8,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3MXS-E"]
[]
[]
[]
[]
["","","","","","3MXS52E4V1B2","3MXS52E4V1B","3MXS52E3V1B"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","47","47"]
["","Refrigeración","","Nom.","dBA","46","46"]
["Accesorios estándar","Manual de instalación","","","","1","1"]
["","Tapón de drenaje","","","","1","1"]
["","Conjunto reductor","","","","1","1"]
["","Placa de ajuste de la dirección del aire","","","","1","1"]
["Refrigerante","Charge","","","TCO2Eq","4.2","4.2"]
["","GWP","","","","2,087.5","2,087.5"]
["","Charge","","","kg","2.0","2.0"]
["","Tipo","","","","R-410A","R-410A"]
["Límites de funcionamiento","Refrigeración","Ambiente","Máx.","°CBS","46","46"]
["","","","Mín.","°CBS","-10","-10"]
["","Calefacción","Ambiente","Máx.","°CBH","18","18"]
["","","","Mín.","°CBH","-15","-15"]
["Piping connections","Diferencia de nivel","Ud. int. – Ud. int.","Máx.","m","7.5","7.5"]
["","","Ud. int. – Ud. ext.","Máx.","m","15","15"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)","0,02 (para longitud de tubería superior a 30 m)"]
["","Longitud de tubería total","Sistema","Real","m","50","50"]
["Compressor","Type","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Dimensiones","Unidad","","Anchura","mm","936","936"]
["","","","Profundidad","mm","300","300"]
["","","","Altura","mm","735","735"]
["Peso","Unidad","","","kg","49","49"]
["Power supply","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","230","230"]
["Notas","","","","","(1) - refrigeración: temp. interior: 27°CBS, 19,0°CBH; temp. exterior 35°CDB; longitud de tubería equivalente: 7,5m","(1) - refrigeración: temp. interior: 27°CBS, 19,0°CBH; temp. exterior 35°CDB; longitud de tubería equivalente: 7,5m"]
["","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5m","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5m"]
["","","","","","(3) - Contiene gases fluorados de efecto invernadero","(3) - Contiene gases fluorados de efecto invernadero"]
["Dimensiones","Unidad","","Altura","mm","","","735"]
["","","","Anchura","mm","","","936"]
["","","","Profundidad","mm","","","300"]
["Peso","Unidad","","","kg","","","49"]
["Compressor","Type","","","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","","","-10"]
["","","","Máx.","°CBS","","","46"]
["","Calefacción","Ambiente","Mín.","°CBH","","","-15"]
["","","","Máx.","°CBH","","","15.5"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","","","46"]
["","Calefacción","","Nom.","dBA","","","47"]
["Refrigerante","Tipo","","","","","","R-410A"]
["","Carga","","","kg","","","2.0"]
["","Carga","","","tCO2Eq","","","4.2"]
["","GWP","","","","","","2087.5"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","","","25"]
["","Carga de refrigerante adicional.","","","kg/m","","","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","","15"]
["","","Ud. int. – Ud. int.","Máx.","m","","","7.5"]
["","Longitud de tubería total","Sistema","Real","m","","","50"]
["Accesorios estándar","Installation manual","","","","","","1"]
["","Drain plug","","","","","","1"]
["","Reducer assembly","","","","","","1"]
["","Air direction adjustment plate","","","","","","1"]
["Alimentación eléctrica","Fase","","","","","","1~"]
["","Frecuencia","","","Hz","","","50"]
["","Tensión","","","V","","","230"]