{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","4MXM-N"]
[]
[]
[]
[]
["","","","","","4MXM68N2V1B (Archived)","4MXM80N2V1B (Archived)"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","24.1","24.1"]
["","","Calefacción","Súper baja","m³/min","24.1","24.1"]
["","","","Súper baja","cfm","851","851.0"]
["","","Calefacción","Súper baja","cfm","851.0","851.0"]
["Dimensiones","Unidad","","Altura","mm","734","734"]
["","","","Anchura","mm","958","958"]
["","","","Profundidad","mm","340","340"]
["Peso","Unidad","","","kg","63","67"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10"]
["","","","Máx.","°CBS","46","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15","-15"]
["","","","Máx.","°CBH","18","18"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","48","49"]
["","Calefacción","","Nom.","dBA","48","49"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","2.00","2.40"]
["","Carga","","","tCO2Eq","1.4","1.6"]
["","GWP","","","","675","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","25","25"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","15"]
["","","Ud. int. – Ud. int.","Máx.","m","7.5","7.5"]
["","Longitud de tubería total","Sistema","Real","m","60","70"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","Drain cap","","","","3","3"]
["","Drain plug","","","","1","1"]
["","Reducer assembly","","","","1","1"]
["","Screw bag","","","","1","1"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]