{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5XXM-A"]
[]
[]
[]
[]
["","","","","","5XXM68A2V1B","5XXM90A2V1B"]
["Dimensiones","Unidad","","Altura","mm","734","734"]
["","","","Anchura","mm","1040","1040"]
["","","","Profundidad","mm","408","408"]
["Peso","Unidad","","","kg","69.0","73.0"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10","-10"]
["","","","Máx.","°CBS","50","50"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","48.0 (2)","52.0 (2)"]
["","Calefacción","","Nom.","dBA","49.0 (2), 51.0 (3)","53.0 (2), 55.0 (3)"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","Carga","","","kg","2.00","2.40"]
["","Carga","","","tCO2Eq","1.35","1.62"]
["","GWP","","","","675","675.0"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","25 (4) (5)","25 (5) (4)"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 30 m)","0,02 (para longitud de tubería superior a 30 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15.0 (5)","15.0 (5)"]
["","","Ud. int. – Ud. int.","Máx.","m","7.5 (5)","7.5 (5)"]
["","Longitud de tubería total","Sistema","Real","m","60","75"]
["Accesorios estándar","Manual de instalación","","","","1","1"]
["","Tapón de drenaje","","","","1","1"]
["","Conjunto reductor","","","","1","1"]
["","Bolsa de tornillos","","","","2","2"]
["Rango de eficiencia energética","","","","","A+++ ~ D","A+++ ~ D"]
["Alimentación eléctrica","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]
["Notas","","","","","(1) - Consulte los esquemas por separado para los límites de funcionamiento","(1) - Consulte los esquemas por separado para los límites de funcionamiento"]
["","","","","","(2) - For DX combination","(2) - For DX combination"]
["","","","","","(3) - For Space heating operation of CHVX07 unit","(3) - For Space heating operation of CHVX07 unit"]
["","","","","","(4) - Para una habitación","(4) - Para una habitación"]
["","","","","","(5) - For combination with FBA71/100/125 refer to installation manual","(5) - For combination with FBA71/100/125 refer to installation manual"]
["","","","","","(6) - Contiene gases fluorados de efecto invernadero","(6) - Contiene gases fluorados de efecto invernadero"]