{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C / AZQS-BY1"]
[]
[]
[]
[]
["","","","","ABQ100CV1 / AZQS100B7Y1B","ABQ125CV1 / AZQS125B7Y1B"]
["Capacidad de refrigeración","Nom.","","kW","9.5","12.1 (1)"]
["Refrigeración de habitaciones","SEER","","","4.65","4.68"]
["","Consumo energético anual","","kWh/a","716","1,550"]
["","Capacidad","Pdesign","kW","9.50","12.1"]
["","Clase de eficiencia energética","","","B"]
["Calefacción de habitaciones (clima medio)","Capacidad","Pdesign","kW","6.78","8.13"]
["","SCOP/A","","","3.80","3.41"]
["","Clase de eficiencia energética","","","A"]
["","Consumo energético anual","","kWh/a","2,498","3,340"]
["Eficiencia nominal","Consumo energético anual","","kWh","1,813"]
["","EER","","","2.62","2.27 (3)"]
["","COP","","","3.42"]
["","Directiva de etiquetado de eficiencia energética","Refrigeración","","D"]
["","","Calefacción","","B"]
["Capacidad de calefacción","Nom.","","kW","10.8","13.5 (2)"]
["Notas","","","","(1) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS; longitud de tubería equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","(2) - Consumo anual de energía de acuerdo con la Directiva de etiquetado energético 2002/31/EC","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 7,5 m; diferencia de nivel 0m"]
["","","","","(3) - SEER y SCOP conforme a EN 14825","(3) - EER/COP conforme a Eurovent 2012, solo para uso fuera de la UE"]
["","","","","(4) - Eficiencia nominal: refrigeración a 35°/27° de carga nominal, calefacción a 7°/20° de carga nominal"]