{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1","ACQ100DV1","ACQ125DV1","ACQ140DV1"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Funcionamiento silencioso","dBA","","36","","41"]
["","","","Bajo","dBA","","38","","43"]
["","Refrigeración","","Funcionamiento silencioso","dBA","","36","","41"]
["","","","Bajo","dBA","","38","","43"]
["","","","Alto","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Accesorios estándar","Manual de instalación","","","","","Manual de instalación","","Manual de instalación"]
["","Manual de uso","","","","","Manual de uso","","Manual de uso"]
["","Tornillos","","","","","Tornillos","","Tornillos"]
["","Arandela","","","","","Arandela","","Arandela"]
["","Mando a distancia sin cable","","","","","Mando a distancia sin cable","","Mando a distancia sin cable"]
["","Rejilla de bloqueo de cubierta","","","","","Rejilla de bloqueo de cubierta","","Rejilla de bloqueo de cubierta"]
["","Batería","","","","","Batería","","Batería"]
["Sistemas de control","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Conexiones de tubería","Líquido","","D.E.","mm","","9.52","","9.52"]
["","Gas","","D.E.","mm","","15.88","","15.88"]
["","Drenaje","","","","","19.05","","19.05"]
["Consumo","Refrigeración","","Nom.","kW","","0.094","","0.137"]
["","Calefacción","","Nom.","kW","","0.094","","0.137"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","56","","60"]
["","Calefacción","","","dBA","","56","","60"]
["Dimensiones","Unidad","","Anchura","mm","","820","","820"]
["","","","Profundidad","mm","","820","","820"]
["","","","Altura","mm","","300","","300"]
["Carcasa","Material","","","","","Acero galvanizado","","Acero galvanizado"]
["Peso","Unidad","","","kg","","39","","39"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","29.2","","34.0"]
["","","","Bajo","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Refrigeración","Bajo","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Alto","m³/min","","29.2","","34.0"]
["","","","Funcionamiento silencioso","m³/min","","17.6","","22.1"]
["","","Refrigeración","Funcionamiento silencioso","m³/min","","17.6","","22.1"]
["Panel decorativo","Peso","","","kg","","4","","4"]
["","Dimensiones","","Altura","mm","","82","","82"]
["","","","Profundidad","mm","","990","","990"]
["","","","Anchura","mm","","990","","990"]
["","Color","","","","","Blanco","","Blanco"]
["Power supply","Phase","","","","","1~","","1~"]
["","Nombre","","","","","V1","","V1"]
["","Frecuencia","","","Hz","","50","","50"]
["","Tensión","","","V","","220-240","","220-240"]
["Ventilador","Caudal de aire","Calefacción","Funcionamiento silencioso","m³/min","15","","22.1"]
["Consumo","Calefacción","","Nom.","kW","0.067","","0.137"]
["","Refrigeración","","Nom.","kW","0.067","","0.137"]
["Ventilador","Caudal de aire","Refrigeración","Funcionamiento silencioso","m³/min","15","","22.1"]
["Carcasa","Material","","","","Acero galvanizado","","Acero galvanizado"]
["Dimensiones","Unidad","","Altura","mm","265","","300"]
["","","","Anchura","mm","820","","820"]
["","","","Profundidad","mm","820","","820"]
["Peso","Unidad","","","kg","31","","39"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Bajo","m³/min","17.6","","26.3"]
["","","Calefacción","Alto","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Bajo","m³/min","17.6","","26.3"]
["Nivel de potencia sonora","Refrigeración","","","dBA","54","","60"]
["","Calefacción","","","dBA","54","","60"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Bajo","dBA","35","","43"]
["","","","Funcionamiento silencioso","dBA","32","","41"]
["","Calefacción","","Alto","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Bajo","dBA","35","","43"]
["","","","Funcionamiento silencioso","dBA","32","","41"]
["Conexiones de tubería","Líquido","","D.E.","mm","9.52","","9.52"]
["","Gas","","D.E.","mm","15.88","","15.88"]
["","Drenaje","","","","19.05","","19.05"]
["Panel decorativo","Dimensiones","","Altura","mm","82","","82"]
["","","","Anchura","mm","990","","990"]
["","","","Profundidad","mm","990","","990"]
["","Peso","","","kg","4","","4"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","ARCWLA","","ARCWLA"]
["","Controlador remoto con cable","","","","ARCWB","","ARCWB"]
["Accesorios estándar","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Alimentación eléctrica","Fase","","","","1~","","1~"]
["","Frecuencia","","","Hz","50","","50"]
["","Tensión","","","V","220-240","","220-240"]