{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXC-B"]
[]
[]
[]
[]
["","","","","","ARXC20BV1B","ARXC25BV1B","ARXC35BV1B","ARXC50BV1B","ARXC60BV1B","ARXC71BV1B"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","45","","","51","54"]
["Refrigerante","Charge","","","TCO2Eq","0.371","","","0.675","0.743"]
["","GWP","","","","675","","","675","675"]
["","Carga","","","kg","0.55","","","1","1.1"]
["","Tipo","","","","R-32","","","R-32","R-32"]
["Conexiones de tubería","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15","","","20","20"]
["","Carga de refrigerante adicional.","","","kg/m","0.017 (para longitud de tubería superior a 7,5m)","","","0.017 (para longitud de tubería superior a 7,5m)","0.017 (para longitud de tubería superior a 7,5m)"]
["Compresor","Tipo","","","","Swing hermético","","","Swing hermético","Swing hermético"]
["Dimensiones","Unidad","","Anchura","mm","658","","","845","845"]
["","","","Profundidad","mm","273","","","300","300"]
["","","","Altura","mm","550","","","615","615"]
["Peso","Unidad","","","kg","24","","","39","39"]
["Power supply","Fase","","","","1~","","","1~","1~"]
["","Frecuencia","","","Hz","50","","","50","50"]
["","Tensión","","","V","220-240","","","220-240","220-240"]
["Dimensiones","Unidad","","Altura","mm","","550","550","","","695"]
["","","","Anchura","mm","","658","658","","","930"]
["","","","Profundidad","mm","","273","273","","","350"]
["Peso","Unidad","","","kg","","24","26","","","45"]
["Compresor","Tipo","","","","","Swing hermético","Swing hermético","","","Swing hermético"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","","10","10","","","-10"]
["","","","Máx.","°CBS","","46","46","","","46"]
["","Calefacción","Ambiente","Mín.","°CBH","","-15","-15","","","-15"]
["","","","Máx.","°CBH","","18","18","","","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","45","46","","","54"]
["Refrigerante","Tipo","","","","","R-32","R-32","","","R-32"]
["","Carga","","","kg","","0.55","0.75","","","1.15"]
["","Carga","","","tCO2Eq","","0.371","0.506","","","0.776"]
["","GWP","","","","","675","675","","","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","","20","20","","","30"]
["","Carga de refrigerante adicional.","","","kg/m","","0.017 (para longitud de tubería superior a 7,5m)","0.017 (para longitud de tubería superior a 7,5m)","","","0.017 (para longitud de tubería superior a 7,5m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","15","15","","","20"]
["Alimentación eléctrica","Fase","","","","","1~","1~","","","1~"]
["","Frecuencia","","","Hz","","50","50","","","50"]
["","Tensión","","","V","","220-240","220-240","","","220-240"]