{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-R9"]
[]
[]
[]
[]
["","","","","","ARXM25R5V1B9","ARXM35R5V1B9"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","","49.0"]
["","Refrigeración","","Nom.","dBA","","49.0"]
["Accesorios estándar","Tapón de drenaje","","","","","1"]
["","Manual de instalación","","","","","1"]
["","Etiqueta de carga de refrigerante","","","","","1"]
["","Etiquetas multilingües para gases de efecto invernadero fluorados","","","","","1"]
["","Precauciones generales de seguridad","","","","","1"]
["Refrigerante","Charge","","","TCO2Eq","","0.52"]
["","GWP","","","","","675"]
["","Carga","","","kg","","0.76"]
["","Tipo","","","","","R-32"]
["Límites de funcionamiento","Refrigeración","Ambiente","Máx.","°CBS","","50 (4), 46 (5)"]
["","","","Mín.","°CBS","","-10"]
["Piping connections","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","","15"]
["","Carga de refrigerante adicional.","","","kg/m","","0,02 (para longitud de tubería superior a 10 m)"]
["Compresor","Type","","","","","Compresor swing herméticamente sellado"]
["Dimensiones","Unidad","","Anchura","mm","","840"]
["","","","Profundidad","mm","","350"]
["","","","Altura","mm","","552"]
["Peso","Unidad","","","kg","","32"]
["Power supply","Phase","","","","","1~"]
["","Frecuencia","","","Hz","","50"]
["","Tensión","","","V","","220-240"]
["Notas","","","","","(1) - Solo posible en combinación con ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Contiene gases fluorados de efecto invernadero"]
["","","","","","(2) - Solo posible en combinación con ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Consulte la ilustración por separado para el rango de funcionamiento"]
["","","","","","","(3) - Consulte en el plano independiente con los datos eléctricos."]
["","","","","","","(4) - Solo posible en combinación con ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","","(5) - Solo posible en combinación con ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]
["Dimensiones","Unidad","","Altura","mm","552"]
["","","","Anchura","mm","840"]
["","","","Profundidad","mm","350"]
["Peso","Unidad","","","kg","32"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","-10"]
["","","","Máx.","°CBS","50 (4), 46 (5)"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","46.0"]
["","Calefacción","","Nom.","dBA","47.0"]
["Refrigerante","Carga","","","kg","0.76"]
["","Carga","","","tCO2Eq","0.52"]
["","GWP","","","","675"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15"]
["Accesorios estándar","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","General safety precautions","","","","1"]
["","Drain plug","","","","1"]
["Alimentación eléctrica","Frecuencia","","","Hz","50"]