{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":65,"n_cols":7,"rows_kept":65,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXS-L3"]
[]
[]
[]
[]
["","","","","","ARXS25L3V1B","ARXS35L3V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","48"]
["","","","Bajo","dBA","","45"]
["Accesorios estándar","1","","","","","550"]
["Refrigerante","Charge","","","kg","","2.5"]
["","Tipo","","","","","1.2"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","","30.1"]
["","","","Súper baja","cfm","","1,063"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","","740"]
["","","Calefacción","Súper baja","rpm","","-15"]
["Límites de funcionamiento","Calefacción","Ambiente","Mín.","°CBH","","20"]
["","","","Máx.","°CBH","","10"]
["Nivel de presión sonora","Refrigeración","","Bajo","dBA","","44"]
["","","","Alto","dBA","","48"]
["Compresor","Tipo","","","","","Compresor swing herméticamente sellado"]
["Dimensiones","Unidad","","Anchura","mm","","285"]
["","","","Profundidad","mm","","612"]
["","","","Altura","mm","","765"]
["Peso","Unidad","","","kg","","34"]
["Ventilador","Caudal de aire","Calefacción","Súper baja","cfm","","904"]
["","","","Súper baja","m³/min","","25.6"]
["Power supply","Fase","","","","","1~"]
["","Frecuencia","","","Hz","","50"]
["","Tensión","","","V","","220-240"]
["Notas","","","","","(1) - 220 V","(1) - Contiene gases fluorados de efecto invernadero"]
["","","","","","(2) - 230V","(2) - 220 V"]
["","","","","","(3) - 240V","(3) - 230V"]
["","","","","","","(4) - 240V"]
["Ventilador","Caudal de aire","Refrigeración","Súper baja","m³/min","30.1"]
["","","Calefacción","Súper baja","m³/min","25.6"]
["","","","Súper baja","cfm","1063"]
["","","Calefacción","Súper baja","cfm","904"]
["Dimensiones","Unidad","","Altura","mm","550"]
["","","","Anchura","mm","765"]
["","","","Profundidad","mm","285"]
["Peso","Unidad","","","kg","34"]
["Motor del ventilador","Velocidad","Refrigeración","Súper baja","rpm","780"]
["","","Calefacción","Súper baja","rpm","740"]
["Compresor","Tipo","","","","Compresor swing herméticamente sellado"]
["Límites de funcionamiento","Refrigeración","Ambiente","Mín.","°CBS","10"]
["","","","Máx.","°CBS","46"]
["","Calefacción","Ambiente","Mín.","°CBH","-15"]
["","","","Máx.","°CBH","18"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","46"]
["","Calefacción","","Alto","dBA","47"]
["","","","Bajo","dBA","44"]
["Refrigerante","Tipo","","","","R-410A"]
["","Carga","","","kg","1.0"]
["","Carga","","","tCO2Eq","2.1"]
["","GWP","","","","2087.5"]
["Conexiones de tubería","Longitud de tubería","Máx.","Ud. ext. – Ud. int.","m","20"]
["","Carga de refrigerante adicional.","","","kg/m","0,02 (para longitud de tubería superior a 10 m)"]
["","Diferencia de nivel","Ud. int. – Ud. ext.","Máx.","m","15"]
["Accesorios estándar","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain plug","","","","1"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]