{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":11,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K2V1B","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","","","","","43"]
["","","","Medio","dBA","","","","","","35"]
["","","","Funcionamiento silencioso","dBA","","","","","","26"]
["","","","Bajo","dBA","","","","","","29"]
["","Refrigeración","","Medio","dBA","","","","","","34"]
["","","","Funcionamiento silencioso","dBA","","","","","","20"]
["","","","Bajo","dBA","","","","","","27"]
["","","","Alto","dBA","","","","","","43"]
["Accesorios estándar","Manual de instalación","","","","","","","","","1"]
["","Manual de uso","","","","","","","","","1"]
["","Mando a distancia por infrarrojos","","","","","","","","","1"]
["","Pilas secas AA","","","","","","","","","2"]
["","Soporte del mando a distancia","","","","","","","","","1"]
["","Placa de montaje","","","","","","","","","1"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","","","","","","","2"]
["","Tornillos de fijación de la unidad interior","","","","","","","","","2"]
["Sistemas de control","Controlador remoto con cable","","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","","ARC480A11"]
["Conexiones de tubería","Liquid","","OD","mm","","","","","","6.35"]
["","Gas","","D.E.","mm","","","","","","9.50"]
["","Drain","","","","","","","","","18"]
["Consumo","Refrigeración","","Nom.","kW","","","","","","0.024"]
["","Calefacción","","Nom.","kW","","","","","","0.029"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","","","","58"]
["","Calefacción","","","dBA","","","","","","58"]
["Dimensiones","Unidad","","Anchura","mm","","","","","","770"]
["","","","Profundidad","mm","","","","","","225"]
["","","","Altura","mm","","","","","","286"]
["Carcasa","Color","","","","","","","","","Blanco"]
["Peso","Unidad","","","kg","","","","","","9.0"]
["Power supply","Fase","","","","","","","","","1~"]
["","Frecuencia","","","Hz","","","","","","50"]
["","Nombre","","","","","","","","","V1"]
["","Tensión","","","V","","","","","","220-240"]
["Notas","","","","","","","","","","(1) - SB: Nivel de ventilador silencioso del ajuste del caudal de aire."]
["Consumo","Refrigeración","","Nom.","kW","0.018","0.018","0.02","0.02","0.024"]
["","Calefacción","","Nom.","kW","0.022","0.022","0.023","0.023","0.029"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","286","286","286","286","286"]
["","","","Anchura","mm","770","770","770","770","770"]
["","","","Profundidad","mm","225","225","225","225","225"]
["Peso","Unidad","","","kg","8.5","8.5","8.5","8.5","9"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","9.9","9.9","10.4","10.4","11.8"]
["","","","Medio","m³/min","7.8","7.8","8","8","8.2"]
["","","","Bajo","m³/min","5.8","5.8","6.1","6.1","6.3"]
["","","","Funcionamiento silencioso","m³/min","4.8","4.8","4.8","4.8","4.9"]
["","","Calefacción","Alto","m³/min","10.9","10.9","11.1","11.1","12.8"]
["","","","Medio","m³/min","8.5","8.5","8.5","8.5","8.5"]
["","","","Bajo","m³/min","6.4","6.4","6.7","6.7","6.9"]
["","","","Funcionamiento silencioso","m³/min","5.2","5.2","5.2","5.2","5.2"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55","55","55","55","58"]
["","Calefacción","","","dBA","55","55","55","55","58"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","39","39","40","40","43"]
["","","","Medio","dBA","33","33","33","33","34"]
["","","","Bajo","dBA","25","25","26","26","27"]
["","","","Funcionamiento silencioso","dBA","20","20","20","20","20"]
["","Calefacción","","Alto","dBA","39","39","40","40","43"]
["","","","Medio","dBA","34","34","34","34","35"]
["","","","Bajo","dBA","28","28","28","28","29"]
["","","","Funcionamiento silencioso","dBA","23","23","23","23","26"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.5","9.5","9.5","9.5"]
["","Drenaje","","","","18","18","18","18","18"]
["Sistemas de control","Infrared remote control","","","","ARC480A11","ARC480A11","","","ARC480A11"]
["Sistemas de control","Controlador remoto con cable","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Accesorios estándar","Installation manual","","","","1","1","1","1","1"]
["","AA dry-cell batteries","","","","2","","2"]
["","Operation manual","","","","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1"]
["Alimentación eléctrica","Nombre","","","","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240","220-240","220-240"]
["Accesorios estándar","AAA dry-cell batteries","","","","","2","","2","2"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","","","ARC480A11","ARC480A11"]
["Accesorios estándar","Titanium apatite photocatalytic air purification filter","","","","","","2"]