{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":9,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXB-C"]
[]
[]
[]
[]
["","","","","","ATXB25C2V1B","ATXB35C2V1B","ATXB50CV1B","ATXB60CV1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","","","","43"]
["","","","Funcionamiento silencioso","dBA","","","","33"]
["","","","Bajo","dBA","","","","37"]
["","Refrigeración","","Funcionamiento silencioso","dBA","","","","33"]
["","","","Muy alto","dBA","","","","46"]
["","","","Bajo","dBA","","","","37"]
["","","","Alto","dBA","","","","43"]
["","","","Nom.","dBA","","","","41"]
["","Refrigeración","","Nom.","dBA","","","","41"]
["Conexiones de tubería","Drain","","","","","","","19.05"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","","61"]
["Dimensiones","Unidad","","Anchura","mm","","","","1,065"]
["","","","Profundidad","mm","","","","224"]
["","","","Altura","mm","","","","310"]
["Carcasa","Color","","","","","","","Blanco"]
["Peso","Unidad","","","kg","","","","14"]
["Power supply","Fase","","","","","","","1~"]
["","Frecuencia","","","Hz","","","","50"]
["","Nombre","","","","","","","V1"]
["","Tensión","","","V","","","","220-240"]
["Notas","","","","","","","","(1) - Todas las unidades han sido probadas y cumplen con la norma ISO 5151 (unidad no conductora) o con la norma ISO 1325 (unidad con conductos)"]
["Ventilador","Caudal de aire","Refrigeración","Nom.","m³/min","7.6","7.7","13.32"]
["Nivel de presión sonora","Refrigeración","","Nom.","dBA","33","34","38"]
["Ventilador","Caudal de aire","Calefacción","Nom.","m³/min","8.0","8.4","13.32"]
["Nivel de presión sonora","Calefacción","","Nom.","dBA","34","35","38"]
["Consumo","Calefacción","","Nom.","kW","0.030","0.030"]
["Carcasa","Color","","","","Blanco","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","283","283","310"]
["","","","Anchura","mm","770","770","1065"]
["","","","Profundidad","mm","216","216","224"]
["Peso","Unidad","","","kg","8","8","14"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","9.2","9.3","15.00"]
["","","","Bajo","m³/min","6.0","6.1","11.82"]
["","","","Funcionamiento silencioso","m³/min","4.8","4.9","10.62"]
["","","Calefacción","Alto","m³/min","9.7","10.1","15.00"]
["","","","Bajo","m³/min","6.3","6.7","11.82"]
["","","","Funcionamiento silencioso","m³/min","5.5","5.7","10.62"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55","58","55"]
["","Calefacción","","","dBA","55","58"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","40","41","40"]
["","","","Bajo","dBA","26","27","35"]
["","","","Funcionamiento silencioso","dBA","21","23","32"]
["","Calefacción","","Alto","dBA","40","41","40"]
["","","","Bajo","dBA","28","29","35"]
["","","","Funcionamiento silencioso","dBA","25","26","32"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.5"]
["","Drenaje","","","","18","18","19.05"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","ARC470A1","ARC470A1"]
["Accesorios estándar","Installation manual","","","","1","1"]
["","AA dry-cell batteries","","","","2","2"]
["","Operation manual","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Infrared remote control","","","","1","1"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Titanium apatite photocatalytic air purification filter","","","","2","2"]
["Alimentación eléctrica","Nombre","","","","V1","V1","V1"]
["","Fase","","","","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50"]
["","Tensión","","","V","220-240","220-240","220-240"]
["Nivel de presión sonora","Refrigeración","","Muy alto","dBA","","","44"]