{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF35C5V1B","ATXF42C5V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","39.0","40.0","","44.0"]
["","","","Medio","dBA","34.0","34.0","","34.0"]
["","","","Funcionamiento silencioso","dBA","21.0","21.0","","22.0"]
["","","","Bajo","dBA","28.0","28.0","","28.0"]
["","Refrigeración","","Medio","dBA","33.0","33.0","","36.0"]
["","","","Funcionamiento silencioso","dBA","20.0","20.0","","22.0"]
["","","","Bajo","dBA","25.0","26.0","","30.0"]
["","","","Alto","dBA","39.0","40.0","","45.0"]
["Accesorios estándar","Manual de instalación","","","","1","1","","1"]
["","Manual de uso","","","","1","1","","1"]
["","Pilas","","","","1","1","","1"]
["","Mando a distancia por infrarrojos","","","","1","1","","1"]
["","Pilas secas AAA","","","","2","2","","2"]
["","Soporte del mando a distancia","","","","1","1","","1"]
["","Placa de montaje","","","","1","1","","1"]
["","Tornillos de fijación de la unidad interior","","","","2","2","","2"]
["Sistemas de control","Controlador remoto con cable","","","","BRC073A1","BRC073A1","","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","","ARC470A1"]
["Conexiones de tubería","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gas","","D.E.","mm","9.50","9.50","","9.50"]
["","Drain","","","","18","18","","18"]
["Consumo","Refrigeración","","Nom.","kW","0.023","0.023","","0.040"]
["","Calefacción","","Nom.","kW","0.023","0.023","","0.040"]
["Nivel de potencia sonora","Refrigeración","","","dBA","53.0","54.0","","59.0"]
["","Calefacción","","","dBA","55.0","55.0","","59.0"]
["Dimensiones","Unidad","","Anchura","mm","770","770","","770"]
["","","","Profundidad","mm","225","225","","225"]
["","","","Altura","mm","286","286","","286"]
["Carcasa","Color","","","","Blanco","Blanco","","Blanco"]
["Peso","Unidad","","","kg","8.00","8.00","","9.00"]
["Power supply","Fase","","","","1~","1~","","1~"]
["","Frecuencia","","","Hz","50","50","","50"]
["","Tensión","","","V","220-440","220-440","","220-440"]
["Consumo","Refrigeración","","Nom.","kW","","","0.029"]
["","Calefacción","","Nom.","kW","","","0.029"]
["Carcasa","Color","","","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","","","286"]
["","","","Anchura","mm","","","770"]
["","","","Profundidad","mm","","","225"]
["Peso","Unidad","","","kg","","","8.5"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","","11.8"]
["","","","Medio","m³/min","","","8"]
["","","","Bajo","m³/min","","","6.4"]
["","","","Funcionamiento silencioso","m³/min","","","4.4"]
["","","Calefacción","Alto","m³/min","","","11.9"]
["","","","Medio","m³/min","","","8.6"]
["","","","Bajo","m³/min","","","6.5"]
["","","","Funcionamiento silencioso","m³/min","","","5.3"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","","54"]
["","Calefacción","","","dBA","","","56"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","","43"]
["","","","Medio","dBA","","","34"]
["","","","Bajo","dBA","","","27"]
["","","","Funcionamiento silencioso","dBA","","","20"]
["","Calefacción","","Alto","dBA","","","40"]
["","","","Medio","dBA","","","35"]
["","","","Bajo","dBA","","","29"]
["","","","Funcionamiento silencioso","dBA","","","21"]
["Conexiones de tubería","Líquido","","D.E.","mm","","","6.35"]
["","Gas","","D.E.","mm","","","9.5"]
["","Drenaje","","","","","","18"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","","","ARC470A1"]
["","Controlador remoto con cable","","","","","","BRC073A1"]
["Accesorios estándar","Installation manual","","","","","","1"]
["","AAA dry-cell batteries","","","","","","2"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","1"]
["","Indoor unit fixing screws","","","","","","2"]
["","Infrared remote control","","","","","","1"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Alimentación eléctrica","Fase","","","","","","1~"]
["","Frecuencia","","","Hz","","","50"]
["","Tensión","","","V","","","220-440"]