{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXL-JV"]
[]
[]
[]
[]
["","","","","ATXL25J2V1B","ATXL35J2V1B"]
["Nivel de presión sonora","Calefacción","Alto","dBA","41","41"]
["","","Funcionamiento silencioso","dBA","26","26"]
["","","Bajo","dBA","29","29"]
["","Refrigeración","Funcionamiento silencioso","dBA","23","23"]
["","","Bajo","dBA","27","27"]
["","","Alto","dBA","41","41"]
["","","Nom.","dBA","35","35"]
["","Refrigeración","Nom.","dBA","34","34"]
["Accesorios estándar","Manual de instalación","","","1","1"]
["","Manual de uso","","","1","1"]
["","Mando a distancia por infrarrojos","","","1","1"]
["","Pilas","","","2","2"]
["","Soporte del mando a distancia","","","1","1"]
["","Placa de montaje","","","1","1"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","2","2"]
["","Tornillos de fijación de la unidad interior","","","2","2"]
["Control systems","Infrared remote control","","","ARC433A87","ARC433A87"]
["Piping connections","Líquido","D.E.","mm","6.35","6.35"]
["","Gas","D.E.","mm","9.5","9.5"]
["","Drenaje","","","18","18"]
["Consumo","Refrigeración","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["","Calefacción","Nom.","kW","0.040 (2), 0.040 (3), 0.040 (4)","0.040 (2), 0.040 (3), 0.040 (4)"]
["Nivel de potencia sonora","Refrigeración","","dBA","57","57"]
["","Calefacción","","dBA","57","57"]
["Dimensiones","Unidad","Anchura","mm","770","770"]
["","","Profundidad","mm","198","198"]
["","","Altura","mm","283","283"]
["Carcasa","Colour","","","Blanco","Blanco"]
["Peso","Unidad","","kg","8","8"]
["Power supply","Fase","","","1~","1~"]
["","Frecuencia","","Hz","50","50"]
["","Nombre","","","V1","V1"]
["","Tensión","","V","220-240","220-240"]
["Notas","","","","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar.","(1) - Cuando esté conectado a una unidad exterior de un sistema Multi, consulte las especificaciones de la unidad que se va a conectar."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]