{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BR00000678"]
[]
[]
[]
[]
["","","","","","BR00000678."]
["Aplicación","","","","","Unidad de suelo"]
["Capacidad","m³/min","","","","33.33"]
["Carcasa","Color","","","","Acabado en acero galvanizado pintado"]
["Dimensiones","Unidad","","Altura","mm","1628"]
["","","","Anchura","mm","720"]
["","","","Profundidad","mm","770"]
["Peso","Unidad","","","kg","150"]
["Superficie máxima de la estancia","m²","","","","133"]
["Operación de purificación de aire","Consumo","","A","kW","0.379"]
["Nivel de presión sonora","Operación de purificación de aire","","Alto","dBA","55.9"]
["Ventilador","Caudal de aire","Operación de purificación de aire","Turbo","m³/h","2300"]
["","","","Alto","m³/h","2000"]
["Dispositivos de seguridad","Elemento","","01","","Interruptor de seguridad (se para el funcionamiento cuando se abre la puerta trasera)"]
["Accesorios estándar","Prefilter selected","","","","1"]
["","HEPA filter selected","","","","1"]
["","Quick Start and Maintenance Guide","","","","1"]
["","Installation and Operation Manual available for download","","","","1"]
["Cable de alimentación eléctrica","m","","","","3"]
["Alimentación eléctrica","Frecuencia","","","Hz","50/60"]
["Corriente de funcionamiento","Operación de purificación de aire","","Alta","A","1.73"]