{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC073"]
[]
[]
[]
[]
["","","","","BRC073A1"]
["Embalaje","Material","","","Cartón_"]
["","Peso","","kg","0.050"]
["Temperatura ambiente","Humedad relativa <","","%","95"]
["","Almacenamiento","Mín.","°C","-20"]
["","","Máx.","°C","70"]
["","Funcionamiento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["Ajuste de temperatura","Resolución","","°C","1"]
["","Rango de punto de ajuste","Refrigeración","°C","18-32"]
["","","Calefacción","°C","10-30"]
["Dimensiones","Unidad con embalaje","Anchura","mm","220"]
["","","Altura","mm","50"]
["","","Profundidad","mm","160"]
["","Unidad","Anchura","mm","120"]
["","","Profundidad","mm","19"]
["","","Altura","mm","120"]
["Carcasa","Tapa de los botones","","","No"]
["","Color","","","Blanco fresco"]
["","LED de funcionamiento","Color","","Verde"]
["LCD","Tipo","","","Punto completo (160 x 255)"]
["","Retroiluminación","Color","","Blanco"]
["","Dimensiones","Anchura","mm","68.85"]
["","","Altura","mm","43.2"]
["Peso","Unidad con embalaje","","kg","0.348"]
["","Unidad","","kg","0.290"]