{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1E53A"]
[]
[]
[]
[]
["","","","","BRC1E53A7"]
["Carcasa","Colour","","","Blanco fresco"]
["","Tapa de los botones","","","No"]
["","LED de funcionamiento","Color","","Verde"]
["Dimensiones","Unidad","Altura","mm","120"]
["","","Anchura","mm","120"]
["","","Profundidad","mm","19"]
["","Unidad con embalaje","Altura","mm","55"]
["","","Anchura","mm","160"]
["","","Profundidad","mm","150"]
["Peso","Unidad","","kg","0.200"]
["","Unidad con embalaje","","kg","0.415"]
["Embalaje","Material","","","Cartón_"]
["","Peso","","kg","0.05"]
["LCD","Tipo","","","Punto completo (160 x 255)"]
["","Dimensiones","Altura","mm","43.2"]
["","","Anchura","mm","68.85"]
["","Retroiluminación","Color","","Blanco"]
["Temperatura ambiente","Funcionamiento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["","Almacenamiento","Mín.","°C","-20"]
["","","Máx.","°C","70"]
["","Humedad relativa <","","%","95"]
["Conexiones de cableado","Longitud de cableado","Máx.","m","500"]
["Reserva para cortes del suministro eléctrico","","","","Sí (el reloj continuará funcionando por un periodo no superior a 48 horas)"]