{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1H52K"]
[]
[]
[]
[]
["","","","","BRC1H52K."]
["Embalaje","Material","","","Cartón"]
["","Peso","","kg","0.0850"]
["Temperatura ambiente","Humedad relativa <","","%","95"]
["","Almacenamiento","Mín.","°C","-20"]
["","","Máx.","°C","70"]
["","Funcionamiento","Mín.","°C","-10"]
["","","Máx.","°C","50"]
["Dimensiones","Unidad con embalaje","Anchura","mm","217"]
["","","Altura","mm","50"]
["","","Profundidad","mm","161"]
["","Unidad","Anchura","mm","85"]
["","","Profundidad","mm","25"]
["","","Altura","mm","85"]
["Carcasa","Tapa de los botones","","","No"]
["","Color","","","Negro"]
["","Operation LED","Colour","","Blue status indicator"]
["LCD","Tipo","","","100 x 150 dots"]
["","Retroiluminación","Color","","Blanco"]
["","Dimensiones","Anchura","mm","28.0"]
["","","Altura","mm","40.7"]
["Peso","Unidad con embalaje","","kg","0.317"]
["","Unidad","","kg","0.110"]
["Conexiones de cableado","Longitud de cableado","Máx.","m","500"]