{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":6,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDK"]
[]
[]
[]
[]
["","","","","BRC1HHDAK (Archived)","BRC1HHDAKA (Archived)"]
["Carcasa","Color","","","Negro","Negro"]
["","Tapa de los botones","","","No","No"]
["","LED de funcionamiento","Color","","Indicador de estado azul","Indicador de estado azul"]
["Dimensiones","Unidad","Altura","mm","85","85"]
["","","Anchura","mm","85","85"]
["","","Profundidad","mm","25","25"]
["","Unidad con embalaje","Altura","mm","50","50"]
["","","Anchura","mm","217","217"]
["","","Profundidad","mm","161","161"]
["Peso","Unidad","","kg","0.110","0.110"]
["","Unidad con embalaje","","kg","0.317","0.317"]
["Embalaje","Material","","","Cartón","Cartón"]
["","Peso","","kg","0.0850","0.0850"]
["LCD","Tipo","","","100 x 150 puntos","100 x 150 puntos"]
["","Dimensiones","Altura","mm","40.7","40.7"]
["","","Anchura","mm","28.0","28.0"]
["","Retroiluminación","Color","","Blanco","Blanco"]
["Temperatura ambiente","Funcionamiento","Mín.","°C","-10","-10"]
["","","Máx.","°C","50","50"]
["","Almacenamiento","Mín.","°C","-20","-20"]
["","","Máx.","°C","70","70"]
["","Temperatura ambiente-=-Humedad relativa <-=-%","","%","95","95"]
["Sistemas de control","Clase de control de temperatura","","","VI","VI"]
["","Contribución a la eficiencia de calefacción de espacios estacional","","%","4.0","4.0"]
["Conexiones de cableado","Longitud de cableado","Máx.","m","500","500"]