{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":13,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHVX-A / 5XXM-A"]
[]
[]
[]
[]
["","","","","","CHVX07S18AJ4V / 5XXM68A2V1B","CHVX07S18AJ9W / 5XXM68A2V1B","CHVX07S23AJ4V / 5XXM68A2V1B","CHVX07S23AJ9W / 5XXM68A2V1B","CHVX07S18AJ4V / 5XXM90A2V1B","CHVX07S18AJ9W / 5XXM90A2V1B","CHVX07S23AJ4V / 5XXM90A2V1B","CHVX07S23AJ9W / 5XXM90A2V1B"]
["Capacidad de calefacción","Nom.","","","kW","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","6.00 (1), 5.90 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)","7.50 (1), 7.80 (2)"]
["Capacidad de refrigeración","Nom.","","","kW","6.50 (1)","6.50 (1)","6.50 (1)","6.50 (1)","7.00 (1)","7.00 (1)","7.00 (1)","7.00 (1)"]
["Consumo","Calefacción","","Nom.","kW","1.33 (1), 2.27 (2)","1.33 (1), 2.27 (2)","1.33 (1), 2.27 (2)","1.33 (1), 2.27 (2)","1.79 (1), 2.89 (2)","1.79 (1), 2.89 (2)","1.79 (1), 2.89 (2)","1.79 (1), 2.89 (2)"]
["","Refrigeración","","Nom.","kW","1.80 (1)","1.80 (1)","1.80 (1)","1.80 (1)","1.94 (1)","1.94 (1)","1.94 (1)","1.94 (1)"]
["COP","","","","","4.50 (1), 2.60 (2)","4.50 (1), 2.60 (2)","4.50 (1), 2.60 (2)","4.50 (1), 2.60 (2)","4.20 (1), 2.70 (2)","4.20 (1), 2.70 (2)","4.20 (1), 2.70 (2)","4.20 (1), 2.70 (2)"]
["EER","","","","","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)","3.61 (1)"]
["Calentamiento de agua caliente sanitaria","General","","Perfil de carga declarado","","L","L","L","L","L","L","L","L"]
["","Clima medio","","Clase de eficiencia energética de calentamiento de agua","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 55°C","General","SCOP","","3.00","3.00","3.00","3.00","3.00","3.00","3.00","3.00"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","Clase de efic. estac. de calef. de habitaciones","","A+","A+","A+","A+","A+","A+","A+","A+"]
["Calefacción de habitaciones","Temperatura del agua de salida en clima medio 35°C","General","SCOP","","4.25","4.25","4.25","4.25","4.10","4.10","4.10","4.10"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 35°C","General","Clase de efic. estac. de calef. de habitaciones","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Rango de eficiencia energética","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Notas","","","","","(2) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(1) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(1) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(1) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(2) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(1) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(1) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH.","(1) - Temperatura del agua de entrada/salida: 7/12 °C; temperatura del aire de entrada: 27 °C BS, 19 °C BH."]