{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","CHYHBH05AAV32","CHYHBH08AFV32"]
["Carcasa","Color","","","","Blanco","Blanco"]
["","Material","","","","Planchas metálicas revestidas","Planchas metálicas revestidas"]
["Dimensiones","Unidad","","Altura","mm","902","902"]
["","","","Anchura","mm","450","450"]
["","","","Profundidad","mm","164","164"]
["Peso","Unidad","","","kg","30.0","30.0"]
["PED","Categoría","","","","","Art3§3, Excluido del alcance de la directiva sobre equipos a presión (PED) por el artículo 1, sección 3.6 de 97/23/EC"]
["Intercambiador de calor del lado del agua","Caudal de agua","Calefacción","Máx.","l/min","23.0 (5)","23.0 (5)"]
["Nivel de potencia sonora","Nom.","","","dBA","42 (6)","42 (6)"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","25 (7)","25 (7)"]
["","","","Máx.","°C","50 (7)","50 (7)"]
["Alimentación eléctrica","Nombre","","","","V3","V3"]
["","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","230","230"]
["Conexiones de cableado","Para conexión con interfaz de usuario","","Cantidad","","2","2"]
["","","","Observación","","0,75 mm² hasta 1,25 mm² (longitud máx. 500 m)","0,75 mm² hasta 1,25 mm² (longitud máx. 500 m)"]
["Notas","","","","","(1) - Solo para la unidad interior","(1) - Solo para la unidad interior"]
["","","","","","(2) - BS/BH 7°C/6°C - LWC 35°C (DT=5°C), caldera derivada","(2) - BS/BH 7°C/6°C - LWC 35°C (DT=5°C), caldera derivada"]
["","","","","","(3) - BS/BH 7°C/6°C - LWC 45℃ (DT=5°C), caldera derivada","(3) - BS/BH 7°C/6°C - LWC 45℃ (DT=5°C), caldera derivada"]
["","","","","","(4) - Min. required","(4) - Min. required"]
["","","","","","(5) - Caldera derivada","(5) - Caldera derivada"]
["","","","","","(6) - Conforme a EN14825","(6) - Conforme a EN14825"]
["","","","","","(7) - Para conocer el rango de funcionamiento de *HYHB* y *HYKOMB33AA, consulte el gráfico del rango de funcionamiento","(7) - Para conocer el rango de funcionamiento de *HYHB* y *HYKOMB33AA, consulte el gráfico del rango de funcionamiento"]