{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":7,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B (Archived)","CTXM15R5V1B (Archived)"]
["Consumo","Refrigeración","","Nom.","kW","0.029","0.029"]
["","Calefacción","","Nom.","kW","0.023","0.023"]
["Carcasa","Color","","","","Blanco","Blanco"]
["Dimensiones","Unidad","","Altura","mm","295","295"]
["","","","Anchura","mm","778","778"]
["","","","Profundidad","mm","272","272"]
["Peso","Unidad","","","kg","10","10"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","10.5","10.5"]
["","","","Medio","m³/min","7.5","7.5"]
["","","","Bajo","m³/min","5.7","5.7"]
["","","","Funcionamiento silencioso","m³/min","4.3","4.3"]
["","","Calefacción","Alto","m³/min","9.3","9.3"]
["","","","Medio","m³/min","8.2","8.2"]
["","","","Bajo","m³/min","6.2","6.2"]
["","","","Funcionamiento silencioso","m³/min","5.1","5.1"]
["Nivel de potencia sonora","Refrigeración","","","dBA","57","57"]
["","Calefacción","","","dBA","54","54"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","41","41"]
["","","","Medio","dBA","33","33"]
["","","","Bajo","dBA","25","25"]
["","","","Funcionamiento silencioso","dBA","19","19"]
["","Calefacción","","Alto","dBA","39","39"]
["","","","Medio","dBA","34","34"]
["","","","Bajo","dBA","26","26"]
["","","","Funcionamiento silencioso","dBA","20","20"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.35","6.35"]
["","Gas","","D.E.","mm","9.5","9.5"]
["","Drenaje","","","","18","18"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","ARC466A67","ARC466A67"]
["","Controlador remoto con cable","","","","BRC073A1","BRC073A1"]
["Accesorios estándar","Manual de instalación","","","","1","1"]
["","Mando a distancia sin cable","","","","1","1"]
["","Pilas secas AAA","","","","2","2"]
["","Kit de adaptador WLAN","","","","1","1"]
["","Manual de uso","","","","1","1"]
["","Filtro desodorizante de apatito de titanio","","","","1","1"]
["","Tornillos de fijación de la unidad interior","","","","2","2"]
["","Placa de montaje","","","","1","1"]
["","Soporte del mando a distancia","","","","1","1"]
["Rango de eficiencia energética","","","","","A+++ ~ D","A+++ ~ D"]
["Alimentación eléctrica","Nombre","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","220-240","220-240"]
["Notas","","","","","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS, 24°CBH; longitud de tubería equivalente 5m","(1) - Refrigeración: temp. interior 27°CBS, 19°CBH; temp. exterior 35°CBS, 24°CBH; longitud de tubería equivalente 5m"]
["","","","","","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m","(2) - Calefacción: temp. interior 20°CBS; temp. exterior 7°CBS, 6°CBH; tubería de refrigerante equivalente 5m"]