{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Nivel de presión sonora","Calefacción","","Alto","dBA","38","","41"]
["","","","Funcionamiento silencioso","dBA","21","","21"]
["","","","Bajo","dBA","28","","30"]
["","Refrigeración","","Funcionamiento silencioso","dBA","21","","21"]
["","","","Bajo","dBA","25","","28"]
["","","","Alto","dBA","37","","42"]
["","","","Nom.","dBA","33"]
["","Refrigeración","","Nom.","dBA","31","","35"]
["Accesorios estándar","Manual de instalación","","","","1","","1"]
["","Manual de uso","","","","1","","1"]
["","Mando a distancia sin cable","","","","1","","1"]
["","Pilas","","","","2","","2"]
["","Soporte del mando a distancia","","","","1","","1"]
["","Placa de montaje","","","","1","","1"]
["","Tornillos de fijación de la unidad interior","","","","2","","2"]
["","Filtro purificador de aire fotocatalítico de apatito de titanio","","","","2","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Piping connections","Líquido","","D.E.","mm","6.35","","6.35"]
["","Gas","","D.E.","mm","9.5","","9.5"]
["","Drenaje","","","","18","","18"]
["Consumo","Refrigeración","","Nom.","kW","0.040","","0.040"]
["","Calefacción","","Nom.","kW","0.040","","0.040"]
["Nivel de potencia sonora","Refrigeración","","","dBA","55","","59"]
["","Calefacción","","","dBA","56","","58"]
["Dimensiones","Unidad","","Anchura","mm","780","","780"]
["","","","Profundidad","mm","215","","215"]
["","","","Altura","mm","289","","289"]
["Carcasa","Colour","","","","Blanco","","Blanco"]
["Peso","Unidad","","","kg","8","","8"]
["Ventilador","Caudal de aire","Calefacción","Alto","m³/min","","","10.1"]
["","","","Bajo","m³/min","","","6.3"]
["","","","Funcionamiento silencioso","m³/min","","","4.3"]
["","","Refrigeración","Bajo","m³/min","","","5.2"]
["","","","Alto","m³/min","","","9.2"]
["","","","Funcionamiento silencioso","m³/min","","","3.9"]
["","","","Nom.","m³/min","","","8.1"]
["","","Refrigeración","Nom.","m³/min","","","7.2"]
["Power supply","Phase","","","","1~","","1~"]
["","Frecuencia","","","Hz","50","","50"]
["","Nombre","","","","V1","","V1"]
["","Tensión","","","V","220-240","","220-240"]
["Notas","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Consumo","Refrigeración","","Nom.","kW","","0.04","","0.040"]
["","Calefacción","","Nom.","kW","","0.04","","0.040"]
["Carcasa","Color","","","","","Blanco","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","","289","","289"]
["","","","Anchura","mm","","780","","780"]
["","","","Profundidad","mm","","215","","215"]
["Peso","Unidad","","","kg","","8","","8.00"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","","7.9","","9.2"]
["","","","Medio","m³/min","","6.3","","7.2"]
["","","","Bajo","m³/min","","4.7","","5.2"]
["","","","Funcionamiento silencioso","m³/min","","3.9","","3.9"]
["","","Calefacción","Alto","m³/min","","9","","10.1"]
["","","","Medio","m³/min","","7.5","","8.1"]
["","","","Bajo","m³/min","","6","","6.3"]
["","","","Funcionamiento silencioso","m³/min","","4.3","","4.3"]
["Nivel de potencia sonora","Refrigeración","","","dBA","","55","","59"]
["","Calefacción","","","dBA","","56","","58"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","","37","","42"]
["","","","Medio","dBA","","31","","35"]
["","","","Bajo","dBA","","25","","28"]
["","","","Funcionamiento silencioso","dBA","","21","","21"]
["","Calefacción","","Alto","dBA","","38","","41"]
["","","","Medio","dBA","","33","","36"]
["","","","Bajo","dBA","","28","","30"]
["","","","Funcionamiento silencioso","dBA","","21","","21"]
["Conexiones de tubería","Líquido","","D.E.","mm","","6.35","","6.35"]
["","Gas","","D.E.","mm","","9.5","","9.50"]
["","Drenaje","","","","","18","","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Accesorios estándar","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Alimentación eléctrica","Nombre","","","","","V1","","V1"]
["","Fase","","","","","1~","","1~"]
["","Frecuencia","","","Hz","","50","","50"]
["","Tensión","","","V","","220-240","","220-240"]