{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CVXM-A9"]
[]
[]
[]
[]
["","","","","","CVXM20A3V1B9"]
["Consumo","Refrigeración","","Nom.","kW","0.02"]
["","Calefacción","","Nom.","kW","0.02"]
["Carcasa","Color","","","","Blanco"]
["Dimensiones","Unidad","","Altura","mm","600"]
["","","","Anchura","mm","750"]
["","","","Profundidad","mm","238"]
["Peso","Unidad","","","kg","17"]
["Ventilador","Caudal de aire","Refrigeración","Alto","m³/min","8.7"]
["","","","Medio","m³/min","7"]
["","","","Bajo","m³/min","4.9"]
["","","","Funcionamiento silencioso","m³/min","4.1"]
["","","Calefacción","Alto","m³/min","9.2"]
["","","","Medio","m³/min","7.2"]
["","","","Bajo","m³/min","5.6"]
["","","","Funcionamiento silencioso","m³/min","4.1"]
["Nivel de potencia sonora","Refrigeración","","","dBA","52"]
["","Calefacción","","","dBA","52"]
["Nivel de presión sonora","Refrigeración","","Alto","dBA","38"]
["","","","Medio","dBA","32"]
["","","","Bajo","dBA","25"]
["","","","Funcionamiento silencioso","dBA","22"]
["","Calefacción","","Alto","dBA","38"]
["","","","Medio","dBA","32"]
["","","","Bajo","dBA","25"]
["","","","Funcionamiento silencioso","dBA","21"]
["Refrigerante","GWP","","","","675"]
["Conexiones de tubería","Líquido","","D.E.","mm","6.4"]
["","Gas","","D.E.","mm","9.5"]
["","Drenaje","","","","VP20 (I.D. 20/O.D. 26)"]
["Sistemas de control","Mando a distancia por infrarrojos","","","","ARC466A66"]
["Sistemas de control","Controlador remoto con cable","","","","BRC073A1"]
["Accesorios estándar","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Alimentación eléctrica","Fase","","","","1~"]
["","Frecuencia","","","Hz","50"]
["","Tensión","","","V","220-240"]