{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCM601A51"]
[]
[]
[]
[]
["","","","","DCM601A51."]
["Temperatura ambiente","Humedad relativa <","","%","85"]
["Número máximo de unidades interiores conectables","","","","64, 512 (1), 2,560 (2)"]
["Consumo","kW","","","0.023"]
["Comunicación","DIII-NET","Cantidad","","1"]
["","Ethernet","Observación","","Acceso Web (100BASE-TX)"]
["","","Cantidad","","1"]
["","Módem","Observación","","Sistema de servicio de red de climatización"]
["Instalación","","","","Solo dirección vertical"]
["Dimensiones","Unidad","Anchura","mm","290"]
["","","Profundidad","mm","50"]
["","","Altura","mm","243"]
["Peso","Unidad","","kg","2.4"]
["Power supply","Frecuencia","","Hz","50/60"]
["","Tensión","","V","AC 100-240"]
["Notas","","","","(1) - Con 7 ITM más adaptadores"]
["","","","","(2) - Con 5 ITM en combinación con integrador ITM"]