{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":13,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EBSXB-D"]
[]
[]
[]
[]
["","","","","","EBSXB11P30DF","EBSXB11P50DF","EBSXB11P30DG","EBSXB11P50DG","EBSXB16P30DF","EBSXB16P50DF","EBSXB16P30DG","EBSXB16P50DG"]
["Carcasa","Color","","","","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)","Blanco Traffic (RAL9016) / Negro Traffic (RAL9017)"]
["","Material","","","","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos","Polipropileno resistente a impactos"]
["Dimensiones","Unidad","","Altura","mm","1,893","1,910","1,893","1,910","1,893","1,910","1,893","1,910"]
["","","","Anchura","mm","594","792","594","792","594","792","594","792"]
["","","","Profundidad","mm","680","817","680","817","680","817","680","817"]
["Peso","Unidad","","","kg","94","117","94","117","94","117","94","117"]
["PED","Categoría","","","","Categoría II","Categoría II","Categoría II","Categoría II","Categoría II","Categoría II","Categoría II","Categoría II"]
["Refrigerante","Tipo","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0"]
["","Carga","","","kg","3.80","3.80","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Carga","","","tCO2Eq","2.57","2.57","2.57","2.57","2.57","2.57","2.57","2.57"]
["Nivel de potencia sonora","Nom.","","","dBA","44.7","44.7","44.7","44.7","49.0","49.0","49.0","49.0"]
["Nivel de presión sonora","Nom.","","","dBA","36.8","36.8","36.8","36.8","40.3","40.3","40.3","40.3"]
["Límites de funcionamiento","Calefacción","Lado del agua","Mín.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Máx.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","Refrigeración","Ambiente","Mín.","°CBS","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","Lado del agua","Mín.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["","","","Máx.","°C","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)","0 (2)"]
["Alimentación eléctrica","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frecuencia","","","Hz","50","50","50","50","50","50","50","50"]
["","Tensión","","","V","230","230","230","230","230","230","230","230"]
["Notas","","","","","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897","(1) - Pérdida de calor conforme a EN12897"]
["","","","","","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano","(2) - Consulte los límites de funcionamiento en plano"]