{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSAX-D9W"]
[]
[]
[]
[]
["","","","","","EGSAX06DA9W","EGSAX10DA9W"]
["Capacidad de calefacción","Mín.","","","kW","0.85","0.85"]
["","Nom.","","","kW","3.35","5.49"]
["","Máx.","","","kW","7.98","9.55"]
["Consumo","Nom.","","","kW","0.74","1.17"]
["COP","","","","","4.51","4.70"]
["Carcasa","Color","","","","Blanco + Negro","Blanco + Negro"]
["","Material","","","","Planchas metálicas revestidas"]
["Dimensiones","Unidad","","Altura","mm","1,891","1,891"]
["","","","Anchura","mm","597","597"]
["","","","Profundidad","mm","666","666"]
["Peso","Unidad","","","kg","222","222"]
["Depósito","Volumen de agua","","","l","180"]
["","Aislamiento","","Pérdida de calor","kWh/24 h","1.2","1.2"]
["","corrosión del depósito","","","","Decapado","Decapado"]
["Refrigerante","Tipo","","","","R-32","R-32"]
["","GWP","","","","675.0","675.0"]
["","Carga","","","kg","1.70","1.70"]
["Rango de funcionamiento","Espacio de instalación","","Mín.","°C","5","5"]
["","","","Máx.","°C","35","35"]
["","Lado de salmuera","","Mín.","°C","-10","-10"]
["","","","Máx.","°C","30","30"]
["","Calefacción","Lado del agua","Min.","°C","5","5"]
["","","","Máx.","°C","65","65"]
["","Agua caliente sanitaria","Lado del agua","Mín.","°C","25","25"]
["","","","Máx.","°C","60","60"]
["Calef. de habitaciones","Temp. del agua de salida, clima medio 55°C","General","SCOP","","3.77 (1)","4.05 (1)"]
["","","","Seasonal space heating eff. class","","A++","A+++"]
["","Temp. agua salida, clima medio 35°C","General","SCOP","","5.18 (1)","5.20 (1)"]
["","","","Clase de efic. estac. de calef. de habitaciones","","A+++","A+++"]
["Power supply","Fase","","","","1~/3~","1~/3~"]
["","Frecuencia","","","Hz","50","50"]
["","Tensión","","","V","230/400","230/400"]
["Corriente","Fusibles recomendados","","","A","16/32","16/32"]
["Notas","","","","","(1) - Conforme a EN14825 y EN14511:2018","(1) - Conforme a EN14825 y EN14511:2018"]
["","","","","","(2) - Consulte el esquema de los límites de funcionamiento: el rango aumenta mediante el calentador auxiliar o el calentador de reserva","(2) - Consulte el esquema de los límites de funcionamiento: el rango aumenta mediante el calentador auxiliar o el calentador de reserva"]